;;- Machine description for GNU compiler, ns32000 Version
;;  Copyright (C) 1988, 1994, 1996 Free Software Foundation, Inc.
;;  Contributed by Michael Tiemann (tiemann@cygnus.com)

;; This file is part of GNU CC.

;; GNU CC is free software; you can redistribute it and/or modify
;; it under the terms of the GNU General Public License as published by
;; the Free Software Foundation; either version 2, or (at your option)
;; any later version.

;; GNU CC is distributed in the hope that it will be useful,
;; but WITHOUT ANY WARRANTY; without even the implied warranty of
;; MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
;; GNU General Public License for more details.

;; You should have received a copy of the GNU General Public License
;; along with GNU CC; see the file COPYING.  If not, write to
;; the Free Software Foundation, 59 Temple Place - Suite 330,
;; Boston, MA 02111-1307, USA.


; BUGS:
;; Insert no-op between an insn with memory read-write operands
;;   following by a scale-indexing operation.
;; The Sequent assembler does not allow addresses to be used
;;   except in insns which explicitly compute an effective address.
;;   I.e., one cannot say "cmpd _p,@_x"
;; Implement unsigned multiplication??

;;- Instruction patterns.  When multiple patterns apply,
;;- the first one in the file is chosen.
;;-
;;- See file "rtl.def" for documentation on define_insn, match_*, et. al.
;;-
;;- cpp macro #define NOTICE_UPDATE_CC in file tm.h handles condition code
;;- updates for most instructions.

;; We don't want to allow a constant operand for test insns because
;; (set (cc0) (const_int foo)) has no mode information.  Such insns will
;; be folded while optimizing anyway.

(define_insn "tstsi"
  [(set (cc0)
	(match_operand:SI 0 "nonimmediate_operand" "rm"))]
  ""
  "*
{ cc_status.flags |= CC_REVERSED;
  operands[1] = const0_rtx;
  return \"cmpqd %1,%0\"; }")

(define_insn "tsthi"
  [(set (cc0)
	(match_operand:HI 0 "nonimmediate_operand" "g"))]
  ""
  "*
{ cc_status.flags |= CC_REVERSED;
  operands[1] = const0_rtx;
  return \"cmpqw %1,%0\"; }")

(define_insn "tstqi"
  [(set (cc0)
	(match_operand:QI 0 "nonimmediate_operand" "g"))]
  ""
  "*
{ cc_status.flags |= CC_REVERSED;
  operands[1] = const0_rtx;
  return \"cmpqb %1,%0\"; }")

(define_insn "tstdf"
  [(set (cc0)
	(match_operand:DF 0 "general_operand" "fmF"))]
  "TARGET_32081"
  "*
{ cc_status.flags |= CC_REVERSED;
  operands[1] = CONST0_RTX (DFmode);
  return \"cmpl %1,%0\"; }")

(define_insn "tstsf"
  [(set (cc0)
	(match_operand:SF 0 "general_operand" "fmF"))]
  "TARGET_32081"
  "*
{ cc_status.flags |= CC_REVERSED;
  operands[1] = CONST0_RTX (SFmode);
  return \"cmpf %1,%0\"; }")

(define_insn "cmpsi"
  [(set (cc0)
	(compare (match_operand:SI 0 "nonimmediate_operand" "rmn")
		 (match_operand:SI 1 "general_operand" "rmn")))]
  ""
  "*
{
  if (GET_CODE (operands[1]) == CONST_INT)
    {
      int i = INTVAL (operands[1]);
      if (i <= 7 && i >= -8)
	{
	  cc_status.flags |= CC_REVERSED;
	  return \"cmpqd %1,%0\";
	}
    }
  cc_status.flags &= ~CC_REVERSED;
  if (GET_CODE (operands[0]) == CONST_INT)
    {
      int i = INTVAL (operands[0]);
      if (i <= 7 && i >= -8)
	return \"cmpqd %0,%1\";
    }
  return \"cmpd %0,%1\";
}")

(define_insn "cmphi"
  [(set (cc0)
	(compare (match_operand:HI 0 "nonimmediate_operand" "g")
		 (match_operand:HI 1 "general_operand" "g")))]
  ""
  "*
{
  if (GET_CODE (operands[1]) == CONST_INT)
    {
      short i = INTVAL (operands[1]);
    if (i <= 7 && i >= -8)
      {
	cc_status.flags |= CC_REVERSED;
	if (INTVAL (operands[1]) > 7)
	  operands[1] = GEN_INT (i);
	return \"cmpqw %1,%0\";
      }
    }
  cc_status.flags &= ~CC_REVERSED;
  if (GET_CODE (operands[0]) == CONST_INT)
    {
      short i = INTVAL (operands[0]);
      if (i <= 7 && i >= -8)
	{
	  if (INTVAL (operands[0]) > 7)
	    operands[0] = GEN_INT (i);
	  return \"cmpqw %0,%1\";
	}
    }
  return \"cmpw %0,%1\";
}")

(define_insn "cmpqi"
  [(set (cc0)
	(compare (match_operand:QI 0 "nonimmediate_operand" "g")
		 (match_operand:QI 1 "general_operand" "g")))]
  ""
  "*
{
  if (GET_CODE (operands[1]) == CONST_INT)
    {
      char i = INTVAL (operands[1]);
      if (i <= 7 && i >= -8)
	{
	  cc_status.flags |= CC_REVERSED;
	  if (INTVAL (operands[1]) > 7)
	    operands[1] = GEN_INT (i);
	  return \"cmpqb %1,%0\";
	}
    }
  cc_status.flags &= ~CC_REVERSED;
  if (GET_CODE (operands[0]) == CONST_INT)
    {
      char i = INTVAL (operands[0]);
      if (i <= 7 && i >= -8)
	{
	  if (INTVAL (operands[0]) > 7)
	    operands[0] = GEN_INT (i);
	  return \"cmpqb %0,%1\";
	}
    }
  return \"cmpb %0,%1\";
}")

(define_insn "cmpdf"
  [(set (cc0)
	(compare (match_operand:DF 0 "general_operand" "fmF")
		 (match_operand:DF 1 "general_operand" "fmF")))]
  "TARGET_32081"
  "cmpl %0,%1")

(define_insn "cmpsf"
  [(set (cc0)
	(compare (match_operand:SF 0 "general_operand" "fmF")
		 (match_operand:SF 1 "general_operand" "fmF")))]
  "TARGET_32081"
  "cmpf %0,%1")

(define_insn "movdf"
  [(set (match_operand:DF 0 "general_operand" "=fg<")
	(match_operand:DF 1 "general_operand" "fFg"))]
  ""
  "*
{
  if (FP_REG_P (operands[0]))
    {
      if (FP_REG_P (operands[1]) || GET_CODE (operands[1]) == CONST_DOUBLE)
	return \"movl %1,%0\";
      if (REG_P (operands[1]))
	{
	  rtx xoperands[2];
	  xoperands[1] = gen_rtx (REG, SImode, REGNO (operands[1]) + 1);
	  output_asm_insn (\"movd %1,tos\", xoperands);
	  output_asm_insn (\"movd %1,tos\", operands);
	  return \"movl tos,%0\";
	}
      return \"movl %1,%0\";
    }
  else if (FP_REG_P (operands[1]))
    {
      if (REG_P (operands[0]))
	{
	  output_asm_insn (\"movl %1,tos\;movd tos,%0\", operands);
	  operands[0] = gen_rtx (REG, SImode, REGNO (operands[0]) + 1);
	  return \"movd tos,%0\";
	}
      else
        return \"movl %1,%0\";
    }
  return output_move_double (operands);
}")

(define_insn "movsf"
  [(set (match_operand:SF 0 "general_operand" "=fg<")
	(match_operand:SF 1 "general_operand" "fFg"))]
  ""
  "*
{
  if (FP_REG_P (operands[0]))
    {
      if (GET_CODE (operands[1]) == REG && REGNO (operands[1]) < 8)
	return \"movd %1,tos\;movf tos,%0\";
      else
	return \"movf %1,%0\";
    }
  else if (FP_REG_P (operands[1]))
    {
      if (REG_P (operands[0]))
	return \"movf %1,tos\;movd tos,%0\";
      return \"movf %1,%0\";
    }
#if 0 /* Someone suggested this for the Sequent.  Is it needed?  */
  else if (GET_CODE (operands[1]) == CONST_DOUBLE)
    return \"movf %1,%0\";
#endif
/* There was a #if 0 around this, but that was erroneous
   for many machines -- rms.  */
#ifndef MOVD_FLOAT_OK
  /* GAS understands floating constants in ordinary movd instructions
     but other assemblers might object.  */
  else if (GET_CODE (operands[1]) == CONST_DOUBLE)
    {
      union {int i[2]; float f; double d;} convrt;
      convrt.i[0] = CONST_DOUBLE_LOW (operands[1]);
      convrt.i[1] = CONST_DOUBLE_HIGH (operands[1]);
      convrt.f = convrt.d;

      /* Is there a better machine-independent way to do this?  */
      operands[1] = GEN_INT (convrt.i[0]);
      return \"movd %1,%0\";
    }
#endif
  else return \"movd %1,%0\";
}")

(define_insn ""
  [(set (match_operand:TI 0 "memory_operand" "=m")
	(match_operand:TI 1 "memory_operand" "m"))]
  ""
  "movmd %1,%0,4")

(define_insn "movdi"
  [(set (match_operand:DI 0 "general_operand" "=g<,*f,g")
	(match_operand:DI 1 "general_operand" "gF,g,*f"))]
  ""
  "*
{
  if (FP_REG_P (operands[0]))
    {
      if (FP_REG_P (operands[1]) || GET_CODE (operands[1]) == CONST_DOUBLE)
	return \"movl %1,%0\";
      if (REG_P (operands[1]))
	{
	  rtx xoperands[2];
	  xoperands[1] = gen_rtx (REG, SImode, REGNO (operands[1]) + 1);
	  output_asm_insn (\"movd %1,tos\", xoperands);
	  output_asm_insn (\"movd %1,tos\", operands);
	  return \"movl tos,%0\";
	}
      return \"movl %1,%0\";
    }
  else if (FP_REG_P (operands[1]))
    {
      if (REG_P (operands[0]))
	{
	  output_asm_insn (\"movl %1,tos\;movd tos,%0\", operands);
	  operands[0] = gen_rtx (REG, SImode, REGNO (operands[0]) + 1);
	  return \"movd tos,%0\";
	}
      else
        return \"movl %1,%0\";
    }
  return output_move_double (operands);
}")

;; This special case must precede movsi.
(define_insn ""
  [(set (reg:SI 17)
	(match_operand:SI 0 "general_operand" "rmn"))]
  ""
  "lprd sp,%0")

(define_insn "movsi"
  [(set (match_operand:SI 0 "general_operand" "=g<,g<,*f,g,x")
	(match_operand:SI 1 "general_operand" "g,?xy,g,*f,rmn"))]
  ""
  "*
{
  extern int flag_pic;						\

  if (FP_REG_P (operands[0]))
    {
      if (GET_CODE (operands[1]) == REG && REGNO (operands[1]) < 8)
	return \"movd %1,tos\;movf tos,%0\";
      else
	return \"movf %1,%0\";
    }
  else if (FP_REG_P (operands[1]))
    {
      if (REG_P (operands[0]))
	return \"movf %1,tos\;movd tos,%0\";
      return \"movf %1,%0\";
    }
  if (GET_CODE (operands[0]) == REG
      && REGNO (operands[0]) == FRAME_POINTER_REGNUM)
    return \"lprd fp,%1\";
  if (GET_CODE (operands[1]) == CONST_DOUBLE)
    operands[1]
      = GEN_INT (CONST_DOUBLE_LOW (operands[1]));
  if (GET_CODE (operands[1]) == CONST_INT)
    {
      int i = INTVAL (operands[1]);
      if (! TARGET_32532)
	{
	  if (i <= 7 && i >= -8)
	    return \"movqd %1,%0\";
	  if (i <= 0x1fffffff && i >= -0x20000000)
#if defined (GNX_V3) || defined (UTEK_ASM)
	    return \"addr %c1,%0\";
#else
	    return \"addr @%c1,%0\";
#endif
	  return \"movd %$%1,%0\";
	}
      else
        return output_move_dconst(i, \"%$%1,%0\");
    }
  else if (GET_CODE (operands[1]) == CONST && ! flag_pic)
    {
	/* Must contain symbols so we don`t know how big it is. In
	 * that case addr might lead to overflow. For PIC symbolic
	 * address loads always have to be done with addr.
	 */
	return \"movd %$%1,%0\";
    }
  else if (GET_CODE (operands[1]) == REG)
    {
      if (REGNO (operands[1]) < 16)
        return \"movd %1,%0\";
      else if (REGNO (operands[1]) == FRAME_POINTER_REGNUM)
	{
	  if (GET_CODE(operands[0]) == REG)
	    return \"sprd fp,%0\";
	  else
	    return \"addr 0(fp),%0\" ;
	}
      else if (REGNO (operands[1]) == STACK_POINTER_REGNUM)
	{
	  if (GET_CODE(operands[0]) == REG)
	    return \"sprd sp,%0\";
	  else
	    return \"addr 0(sp),%0\" ;
	}
      else abort ();
    }
  else if (GET_CODE (operands[1]) == MEM)
    return \"movd %1,%0\";

  /* Check if this effective address can be
     calculated faster by pulling it apart.  */
  if (REG_P (operands[0])
      && GET_CODE (operands[1]) == MULT
      && GET_CODE (XEXP (operands[1], 1)) == CONST_INT
      && (INTVAL (XEXP (operands[1], 1)) == 2
	  || INTVAL (XEXP (operands[1], 1)) == 4))
    {
      rtx xoperands[3];
      xoperands[0] = operands[0];
      xoperands[1] = XEXP (operands[1], 0);
      xoperands[2] = GEN_INT (INTVAL (XEXP (operands[1], 1)) >> 1);
      return output_shift_insn (xoperands);
    }
  return \"addr %a1,%0\";
}")

(define_insn "movhi"
  [(set (match_operand:HI 0 "general_operand" "=g<,*f,g")
	(match_operand:HI 1 "general_operand" "g,g,*f"))]
  ""
  "*
{
  if (GET_CODE (operands[1]) == CONST_INT)
    {
      short i = INTVAL (operands[1]);
      if (i <= 7 && i >= -8)
	{
	  if (INTVAL (operands[1]) > 7)
	    operands[1] =
	      GEN_INT (i);
	  return \"movqw %1,%0\";
	}
	return \"movw %1,%0\";
    }
  else if (FP_REG_P (operands[0]))
    {
      if (GET_CODE (operands[1]) == REG && REGNO (operands[1]) < 8)
	return \"movwf %1,tos\;movf tos,%0\";
      else
	return \"movwf %1,%0\";
    }
  else if (FP_REG_P (operands[1]))
    {
      if (REG_P (operands[0]))
	return \"movf %1,tos\;movd tos,%0\";
      return \"movf %1,%0\";
    }
  else
     return \"movw %1,%0\";
}")

(define_insn "movstricthi"
  [(set (strict_low_part (match_operand:HI 0 "general_operand" "+r"))
	(match_operand:HI 1 "general_operand" "g"))]
  ""
  "*
{
  if (GET_CODE (operands[1]) == CONST_INT
      && INTVAL(operands[1]) <= 7 && INTVAL(operands[1]) >= -8)
    return \"movqw %1,%0\";
  return \"movw %1,%0\";
}")

(define_insn "movqi"
  [(set (match_operand:QI 0 "general_operand" "=g<,*f,g")
	(match_operand:QI 1 "general_operand" "g,g,*f"))]
  ""
  "*
{ if (GET_CODE (operands[1]) == CONST_INT)
    {
      char char_val = (char)INTVAL (operands[1]);
      if (char_val <= 7 && char_val >= -8)
	{
	  if (INTVAL (operands[1]) > 7)
	    operands[1] =
	      GEN_INT (char_val);
	  return \"movqb %1,%0\";
	}
	return \"movb %1,%0\";
    }
  else if (FP_REG_P (operands[0]))
    {
      if (GET_CODE (operands[1]) == REG && REGNO (operands[1]) < 8)
	return \"movbf %1,tos\;movf tos,%0\";
      else
	return \"movbf %1,%0\";
    }
  else if (FP_REG_P (operands[1]))
    {
      if (REG_P (operands[0]))
	return \"movf %1,tos\;movd tos,%0\";
      return \"movf %1,%0\";
    }
  else
     return \"movb %1,%0\";
}")

(define_insn "movstrictqi"
  [(set (strict_low_part (match_operand:QI 0 "general_operand" "+r"))
	(match_operand:QI 1 "general_operand" "g"))]
  ""
  "*
{
  if (GET_CODE (operands[1]) == CONST_INT
      && INTVAL(operands[1]) < 8 && INTVAL(operands[1]) > -9)
    return \"movqb %1,%0\";
  return \"movb %1,%0\";
}")

;; This is here to accept 4 arguments and pass the first 3 along
;; to the movstrsi1 pattern that really does the work.
(define_expand "movstrsi"
  [(set (match_operand:BLK 0 "general_operand" "=g")
	(match_operand:BLK 1 "general_operand" "g"))
   (use (match_operand:SI 2 "general_operand" "rmn"))
   (match_operand 3 "" "")]
  ""
  "
  emit_insn (gen_movstrsi1 (operands[0], operands[1], operands[2]));
  DONE;
")

;; The definition of this insn does not really explain what it does,
;; but it should suffice
;; that anything generated as this insn will be recognized as one
;; and that it won't successfully combine with anything.
(define_insn "movstrsi1"
  [(set (match_operand:BLK 0 "general_operand" "=g")
	(match_operand:BLK 1 "general_operand" "g"))
   (use (match_operand:SI 2 "general_operand" "rmn"))
   (clobber (reg:SI 0))
   (clobber (reg:SI 1))
   (clobber (reg:SI 2))]
  ""
  "*
{
  if (GET_CODE (operands[0]) != MEM || GET_CODE (operands[1]) != MEM)
    abort ();
  operands[0] = XEXP (operands[0], 0);
  operands[1] = XEXP (operands[1], 0);
  if (GET_CODE (operands[0]) == MEM)
    if (GET_CODE (operands[1]) == MEM)
      output_asm_insn (\"movd %0,r2\;movd %1,r1\", operands);
    else
      output_asm_insn (\"movd %0,r2\;addr %a1,r1\", operands);
  else if (GET_CODE (operands[1]) == MEM)
    output_asm_insn (\"addr %a0,r2\;movd %1,r1\", operands);
  else
    output_asm_insn (\"addr %a0,r2\;addr %a1,r1\", operands);

#ifdef UTEK_ASM
  if (GET_CODE (operands[2]) == CONST_INT && (INTVAL (operands[2]) & 0x3) == 0)
    {
      operands[2] = GEN_INT (INTVAL (operands[2]) >> 2);
      if ((unsigned) INTVAL (operands[2]) <= 7)
	return \"movqd %2,r0\;movsd $0\";
      else 
	return \"movd %2,r0\;movsd $0\";
    }
  else
    {
      return \"movd %2,r0\;movsb $0\";
    }
#else
  if (GET_CODE (operands[2]) == CONST_INT && (INTVAL (operands[2]) & 0x3) == 0)
    {
      operands[2] = GEN_INT (INTVAL (operands[2]) >> 2);
      if ((unsigned) INTVAL (operands[2]) <= 7)
	return \"movqd %2,r0\;movsd\";
      else 
	return \"movd %2,r0\;movsd\";
    }
  else
    {
      return \"movd %2,r0\;movsb\";
    }
#endif
}")

;; Extension and truncation insns.
;; Those for integer source operand
;; are ordered widest source type first.

(define_insn "truncsiqi2"
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(truncate:QI (match_operand:SI 1 "nonimmediate_operand" "rmn")))]
  ""
  "movb %1,%0")

(define_insn "truncsihi2"
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(truncate:HI (match_operand:SI 1 "nonimmediate_operand" "rmn")))]
  ""
  "movw %1,%0")

(define_insn "trunchiqi2"
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(truncate:QI (match_operand:HI 1 "nonimmediate_operand" "g")))]
  ""
  "movb %1,%0")

(define_insn "extendhisi2"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(sign_extend:SI (match_operand:HI 1 "nonimmediate_operand" "g")))]
  ""
  "movxwd %1,%0")

(define_insn "extendqihi2"
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(sign_extend:HI (match_operand:QI 1 "nonimmediate_operand" "g")))]
  ""
  "movxbw %1,%0")

(define_insn "extendqisi2"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(sign_extend:SI (match_operand:QI 1 "nonimmediate_operand" "g")))]
  ""
  "movxbd %1,%0")

(define_insn "extendsfdf2"
  [(set (match_operand:DF 0 "general_operand" "=fm<")
	(float_extend:DF (match_operand:SF 1 "general_operand" "fmF")))]
  "TARGET_32081"
  "movfl %1,%0")

(define_insn "truncdfsf2"
  [(set (match_operand:SF 0 "general_operand" "=fm<")
	(float_truncate:SF (match_operand:DF 1 "general_operand" "fmF")))]
  "TARGET_32081"
  "movlf %1,%0")

(define_insn "zero_extendhisi2"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(zero_extend:SI (match_operand:HI 1 "nonimmediate_operand" "g")))]
  ""
  "movzwd %1,%0")

(define_insn "zero_extendqihi2"
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(zero_extend:HI (match_operand:QI 1 "nonimmediate_operand" "g")))]
  ""
  "movzbw %1,%0")

(define_insn "zero_extendqisi2"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(zero_extend:SI (match_operand:QI 1 "nonimmediate_operand" "g")))]
  ""
  "movzbd %1,%0")

;; Fix-to-float conversion insns.
;; Note that the ones that start with SImode come first.
;; That is so that an operand that is a CONST_INT
;; (and therefore lacks a specific machine mode).
;; will be recognized as SImode (which is always valid)
;; rather than as QImode or HImode.

;; Rumor has it that the National part does not correctly convert
;; constant ints to floats.  This conversion is therefore disabled.
;; A register must be used to perform the conversion.

(define_insn "floatsisf2"
  [(set (match_operand:SF 0 "general_operand" "=fm<")
	(float:SF (match_operand:SI 1 "general_operand" "rm")))]
  "TARGET_32081"
  "movdf %1,%0")

(define_insn "floatsidf2"
  [(set (match_operand:DF 0 "general_operand" "=fm<")
	(float:DF (match_operand:SI 1 "general_operand" "rm")))]
  "TARGET_32081"
  "movdl %1,%0")

(define_insn "floathisf2"
  [(set (match_operand:SF 0 "general_operand" "=fm<")
	(float:SF (match_operand:HI 1 "general_operand" "rm")))]
  "TARGET_32081"
  "movwf %1,%0")

(define_insn "floathidf2"
  [(set (match_operand:DF 0 "general_operand" "=fm<")
	(float:DF (match_operand:HI 1 "general_operand" "rm")))]
  "TARGET_32081"
  "movwl %1,%0")

(define_insn "floatqisf2"
  [(set (match_operand:SF 0 "general_operand" "=fm<")
	(float:SF (match_operand:QI 1 "general_operand" "rm")))]
  "TARGET_32081"
  "movbf %1,%0")

; Some assemblers warn that this insn doesn't work.
; Maybe they know something we don't.
;(define_insn "floatqidf2"
;  [(set (match_operand:DF 0 "general_operand" "=fm<")
;	(float:DF (match_operand:QI 1 "general_operand" "rm")))]
;  "TARGET_32081"
;  "movbl %1,%0")

;; Float-to-fix conversion insns.
;; The sequent compiler always generates "trunc" insns.

(define_insn "fixsfqi2"
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(fix:QI (fix:SF (match_operand:SF 1 "general_operand" "fm"))))]
  "TARGET_32081"
  "truncfb %1,%0")

(define_insn "fixsfhi2"
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(fix:HI (fix:SF (match_operand:SF 1 "general_operand" "fm"))))]
  "TARGET_32081"
  "truncfw %1,%0")

(define_insn "fixsfsi2"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(fix:SI (fix:SF (match_operand:SF 1 "general_operand" "fm"))))]
  "TARGET_32081"
  "truncfd %1,%0")

(define_insn "fixdfqi2"
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(fix:QI (fix:DF (match_operand:DF 1 "general_operand" "fm"))))]
  "TARGET_32081"
  "trunclb %1,%0")

(define_insn "fixdfhi2"
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(fix:HI (fix:DF (match_operand:DF 1 "general_operand" "fm"))))]
  "TARGET_32081"
  "trunclw %1,%0")

(define_insn "fixdfsi2"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(fix:SI (fix:DF (match_operand:DF 1 "general_operand" "fm"))))]
  "TARGET_32081"
  "truncld %1,%0")

;; Unsigned

(define_insn "fixunssfqi2"
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(unsigned_fix:QI (fix:SF (match_operand:SF 1 "general_operand" "fm"))))]
  "TARGET_32081"
  "truncfb %1,%0")

(define_insn "fixunssfhi2"
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(unsigned_fix:HI (fix:SF (match_operand:SF 1 "general_operand" "fm"))))]
  "TARGET_32081"
  "truncfw %1,%0")

(define_insn "fixunssfsi2"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(unsigned_fix:SI (fix:SF (match_operand:SF 1 "general_operand" "fm"))))]
  "TARGET_32081"
  "truncfd %1,%0")

(define_insn "fixunsdfqi2"
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(unsigned_fix:QI (fix:DF (match_operand:DF 1 "general_operand" "fm"))))]
  "TARGET_32081"
  "trunclb %1,%0")

(define_insn "fixunsdfhi2"
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(unsigned_fix:HI (fix:DF (match_operand:DF 1 "general_operand" "fm"))))]
  "TARGET_32081"
  "trunclw %1,%0")

(define_insn "fixunsdfsi2"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(unsigned_fix:SI (fix:DF (match_operand:DF 1 "general_operand" "fm"))))]
  "TARGET_32081"
  "truncld %1,%0")

;;; These are not yet used by GCC
(define_insn "fix_truncsfqi2"
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(fix:QI (match_operand:SF 1 "general_operand" "fm")))]
  "TARGET_32081"
  "truncfb %1,%0")

(define_insn "fix_truncsfhi2"
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(fix:HI (match_operand:SF 1 "general_operand" "fm")))]
  "TARGET_32081"
  "truncfw %1,%0")

(define_insn "fix_truncsfsi2"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(fix:SI (match_operand:SF 1 "general_operand" "fm")))]
  "TARGET_32081"
  "truncfd %1,%0")

(define_insn "fix_truncdfqi2"
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(fix:QI (match_operand:DF 1 "general_operand" "fm")))]
  "TARGET_32081"
  "trunclb %1,%0")

(define_insn "fix_truncdfhi2"
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(fix:HI (match_operand:DF 1 "general_operand" "fm")))]
  "TARGET_32081"
  "trunclw %1,%0")

(define_insn "fix_truncdfsi2"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(fix:SI (match_operand:DF 1 "general_operand" "fm")))]
  "TARGET_32081"
  "truncld %1,%0")

;;- All kinds of add instructions.

(define_insn "adddf3"
  [(set (match_operand:DF 0 "general_operand" "=fm")
	(plus:DF (match_operand:DF 1 "general_operand" "%0")
		 (match_operand:DF 2 "general_operand" "fmF")))]
  "TARGET_32081"
  "addl %2,%0")


(define_insn "addsf3"
  [(set (match_operand:SF 0 "general_operand" "=fm")
	(plus:SF (match_operand:SF 1 "general_operand" "%0")
		 (match_operand:SF 2 "general_operand" "fmF")))]
  "TARGET_32081"
  "addf %2,%0")

(define_insn ""
  [(set (reg:SI 17)
	(plus:SI (reg:SI 17)
		 (match_operand:SI 0 "immediate_operand" "i")))]
  "GET_CODE (operands[0]) == CONST_INT"
  "*
{
#ifndef SEQUENT_ADJUST_STACK
  if (TARGET_32532)
    if (INTVAL (operands[0]) == 8)
      return \"cmpd tos,tos\";
  if (TARGET_32532 || TARGET_32332)
    if (INTVAL (operands[0]) == 4)
      return \"cmpqd %$0,tos\";
#endif
  if (! TARGET_32532)
    {
      if (INTVAL (operands[0]) < 64 && INTVAL (operands[0]) > -64)
        return \"adjspb %$%n0\";
      else if (INTVAL (operands[0]) < 8192 && INTVAL (operands[0]) >= -8192)
        return \"adjspw %$%n0\";
    }
  return \"adjspd %$%n0\";
}")

(define_insn ""
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(plus:SI (reg:SI 16)
		 (match_operand:SI 1 "immediate_operand" "i")))]
  "GET_CODE (operands[1]) == CONST_INT"
  "addr %c1(fp),%0")

(define_insn ""
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(plus:SI (reg:SI 17)
		 (match_operand:SI 1 "immediate_operand" "i")))]
  "GET_CODE (operands[1]) == CONST_INT"
  "addr %c1(sp),%0")

(define_insn "adddi3"
  [(set (match_operand:DI 0 "general_operand" "=ro")
	(plus:DI (match_operand:DI 1 "general_operand" "%0")
		 (match_operand:DI 2 "general_operand" "ron")))]
  ""
  "*
{
  rtx low[3], high[3], xops[4];
  split_di (operands, 3, low, high);
  xops[0] = low[0];
  xops[1] = high[0];
  xops[2] = low[2];
  xops[3] = high[2];

  if (GET_CODE (xops[2]) == CONST_INT)
    {
      int i = INTVAL (xops[2]);

      if (i <= 7 && i >= -8) 
        {
          if (i == 0)
	    {
	      i = INTVAL (xops[3]);
	      if (i <= 7 && i >= -8)
                output_asm_insn (\"addqd %$%3,%1\", xops);
	      else
                output_asm_insn (\"addd %$%3,%1\", xops);
	    }
	  else
	    {
              output_asm_insn (\"addqd %$%2,%0\", xops);
              output_asm_insn (\"addcd %$%3,%1\", xops);
	    }
	  return \"\";
	}
    }
  output_asm_insn (\"addd %2,%0\", xops);
  output_asm_insn (\"addcd %3,%1\", xops);
  return \"\";
}")

(define_insn "addsi3"
  [(set (match_operand:SI 0 "general_operand" "=g,=g&<")
	(plus:SI (match_operand:SI 1 "general_operand" "%0,r")
		 (match_operand:SI 2 "general_operand" "rmn,n")))]
  ""
  "*
{
  if (which_alternative == 1)
    {
      int i = INTVAL (operands[2]);
      if (NS32K_DISPLACEMENT_P (i))
	return \"addr %c2(%1),%0\";
      else
	return \"movd %1,%0\;addd %2,%0\";
    }
  if (GET_CODE (operands[2]) == CONST_INT)
    {
      int i = INTVAL (operands[2]);

      if (i <= 7 && i >= -8)
	return \"addqd %2,%0\";
      else if (! TARGET_32532 && GET_CODE (operands[0]) == REG
	       && i <= 0x1fffffff && i >= -0x20000000)
	return \"addr %c2(%0),%0\";
    }
  return \"addd %2,%0\";
}")

(define_insn "addhi3"
  [(set (match_operand:HI 0 "general_operand" "=g")
	(plus:HI (match_operand:HI 1 "general_operand" "%0")
		 (match_operand:HI 2 "general_operand" "g")))]
  ""
  "*
{ if (GET_CODE (operands[2]) == CONST_INT)
    {
      int i = INTVAL (operands[2]);
      if (i <= 7 && i >= -8)
	return \"addqw %2,%0\";
    }
  return \"addw %2,%0\";
}")

(define_insn ""
  [(set (strict_low_part (match_operand:HI 0 "general_operand" "=r"))
	(plus:HI (match_operand:HI 1 "general_operand" "0")
		 (match_operand:HI 2 "general_operand" "g")))]
  ""
  "*
{
  if (GET_CODE (operands[1]) == CONST_INT
      && INTVAL (operands[1]) >-9 && INTVAL(operands[1]) < 8)
    return \"addqw %2,%0\";
  return \"addw %2,%0\";
}")

(define_insn "addqi3"
  [(set (match_operand:QI 0 "general_operand" "=g")
	(plus:QI (match_operand:QI 1 "general_operand" "%0")
		 (match_operand:QI 2 "general_operand" "g")))]
  ""
  "*
{ if (GET_CODE (operands[2]) == CONST_INT)
    {
      int i = INTVAL (operands[2]);
      if (i <= 7 && i >= -8)
	return \"addqb %2,%0\";
    }
  return \"addb %2,%0\";
}")

(define_insn ""
  [(set (strict_low_part (match_operand:QI 0 "general_operand" "=r"))
	(plus:QI (match_operand:QI 1 "general_operand" "0")
		 (match_operand:QI 2 "general_operand" "g")))]
  ""
  "*
{
  if (GET_CODE (operands[1]) == CONST_INT
      && INTVAL (operands[1]) >-9 && INTVAL(operands[1]) < 8)
    return \"addqb %2,%0\";
  return \"addb %2,%0\";
}")

;;- All kinds of subtract instructions.

(define_insn "subdf3"
  [(set (match_operand:DF 0 "general_operand" "=fm")
	(minus:DF (match_operand:DF 1 "general_operand" "0")
		  (match_operand:DF 2 "general_operand" "fmF")))]
  "TARGET_32081"
  "subl %2,%0")

(define_insn "subsf3"
  [(set (match_operand:SF 0 "general_operand" "=fm")
	(minus:SF (match_operand:SF 1 "general_operand" "0")
		  (match_operand:SF 2 "general_operand" "fmF")))]
  "TARGET_32081"
  "subf %2,%0")

(define_insn ""
  [(set (reg:SI 17)
	(minus:SI (reg:SI 17)
		  (match_operand:SI 0 "immediate_operand" "i")))]
  "GET_CODE (operands[0]) == CONST_INT"
  "*
{
  if (! TARGET_32532 && GET_CODE(operands[0]) == CONST_INT 
      && INTVAL(operands[0]) < 64 && INTVAL(operands[0]) > -64)
    return \"adjspb %$%0\";
  return \"adjspd %$%0\";
}")

(define_insn "subdi3"
  [(set (match_operand:DI 0 "general_operand" "=ro")
	(minus:DI (match_operand:DI 1 "general_operand" "0")
		  (match_operand:DI 2 "general_operand" "ron")))]
  ""
  "*
{
  rtx low[3], high[3], xops[4];
  split_di (operands, 3, low, high);
  xops[0] = low[0];
  xops[1] = high[0];
  xops[2] = low[2];
  xops[3] = high[2];

  if (GET_CODE (xops[2]) == CONST_INT)
    {
      int i = INTVAL (xops[2]);

      if (i <= 8 && i >= -7)
        {
          if (i == 0)
	    {
	      i = INTVAL (xops[3]);
	      if (i <= 8 && i >= -7)
                output_asm_insn (\"addqd %$%n3,%1\", xops);
	      else
                output_asm_insn (\"subd %$%3,%1\", xops);
	    }
	  else
	    {
              output_asm_insn (\"addqd %$%n2,%0\", xops);
              output_asm_insn (\"subcd %$%3,%1\", xops);
	    }
	  return \"\";
	}
    }
  output_asm_insn (\"subd %2,%0\", xops);
  output_asm_insn (\"subcd %3,%1\", xops);
  return \"\";
}")

(define_insn "subsi3"
  [(set (match_operand:SI 0 "general_operand" "=g")
	(minus:SI (match_operand:SI 1 "general_operand" "0")
		  (match_operand:SI 2 "general_operand" "rmn")))]
  ""
  "*
{ if (GET_CODE (operands[2]) == CONST_INT)
    {
      int i = INTVAL (operands[2]);

      if (i <= 8 && i >= -7)
        return \"addqd %$%n2,%0\";
    }
  return \"subd %2,%0\";
}")

(define_insn "subhi3"
  [(set (match_operand:HI 0 "general_operand" "=g")
	(minus:HI (match_operand:HI 1 "general_operand" "0")
		  (match_operand:HI 2 "general_operand" "g")))]
  ""
  "*
{ if (GET_CODE (operands[2]) == CONST_INT)
    {
      int i = INTVAL (operands[2]);

      if (i <= 8 && i >= -7)
        return \"addqw %$%n2,%0\";
    }
  return \"subw %2,%0\";
}")

(define_insn ""
  [(set (strict_low_part (match_operand:HI 0 "general_operand" "=r"))
	(minus:HI (match_operand:HI 1 "general_operand" "0")
		  (match_operand:HI 2 "general_operand" "g")))]
  ""
  "*
{
  if (GET_CODE (operands[1]) == CONST_INT
      && INTVAL (operands[1]) >-8 && INTVAL(operands[1]) < 9)
    return \"addqw %$%n2,%0\";
  return \"subw %2,%0\";
}")

(define_insn "subqi3"
  [(set (match_operand:QI 0 "general_operand" "=g")
	(minus:QI (match_operand:QI 1 "general_operand" "0")
		  (match_operand:QI 2 "general_operand" "g")))]
  ""
  "*
{ if (GET_CODE (operands[2]) == CONST_INT)
    {
      int i = INTVAL (operands[2]);

      if (i <= 8 && i >= -7)
	return \"addqb %$%n2,%0\";
    }
  return \"subb %2,%0\";
}")

(define_insn ""
  [(set (strict_low_part (match_operand:QI 0 "general_operand" "=r"))
	(minus:QI (match_operand:QI 1 "general_operand" "0")
		  (match_operand:QI 2 "general_operand" "g")))]
  ""
  "*
{
  if (GET_CODE (operands[1]) == CONST_INT
      && INTVAL (operands[1]) >-8 && INTVAL(operands[1]) < 9)
    return \"addqb %$%n2,%0\";
  return \"subb %2,%0\";
}")

;;- Multiply instructions.

(define_insn "muldf3"
  [(set (match_operand:DF 0 "general_operand" "=fm")
	(mult:DF (match_operand:DF 1 "general_operand" "%0")
		 (match_operand:DF 2 "general_operand" "fmF")))]
  "TARGET_32081"
  "mull %2,%0")

(define_insn "mulsf3"
  [(set (match_operand:SF 0 "general_operand" "=fm")
	(mult:SF (match_operand:SF 1 "general_operand" "%0")
		 (match_operand:SF 2 "general_operand" "fmF")))]
  "TARGET_32081"
  "mulf %2,%0")

(define_insn "mulsi3"
  [(set (match_operand:SI 0 "general_operand" "=g")
	(mult:SI (match_operand:SI 1 "general_operand" "%0")
		 (match_operand:SI 2 "general_operand" "rmn")))]
  ""
  "muld %2,%0")

(define_insn "mulhi3"
  [(set (match_operand:HI 0 "general_operand" "=g")
	(mult:HI (match_operand:HI 1 "general_operand" "%0")
		 (match_operand:HI 2 "general_operand" "g")))]
  ""
  "mulw %2,%0")

(define_insn "mulqi3"
  [(set (match_operand:QI 0 "general_operand" "=g")
	(mult:QI (match_operand:QI 1 "general_operand" "%0")
		 (match_operand:QI 2 "general_operand" "g")))]
  ""
  "mulb %2,%0")

(define_insn "umulsidi3"
  [(set (match_operand:DI 0 "general_operand" "=g")
	(mult:DI (zero_extend:DI
		  (match_operand:SI 1 "nonimmediate_operand" "0"))
		 (zero_extend:DI
		  (match_operand:SI 2 "nonimmediate_operand" "rmn"))))]
  ""
  "meid %2,%0")

;;- Divide instructions.

(define_insn "divdf3"
  [(set (match_operand:DF 0 "general_operand" "=fm")
	(div:DF (match_operand:DF 1 "general_operand" "0")
		(match_operand:DF 2 "general_operand" "fmF")))]
  "TARGET_32081"
  "divl %2,%0")

(define_insn "divsf3"
  [(set (match_operand:SF 0 "general_operand" "=fm")
	(div:SF (match_operand:SF 1 "general_operand" "0")
		(match_operand:SF 2 "general_operand" "fmF")))]
  "TARGET_32081"
  "divf %2,%0")

(define_insn "divsi3"
  [(set (match_operand:SI 0 "general_operand" "=g")
	(div:SI (match_operand:SI 1 "general_operand" "0")
		(match_operand:SI 2 "general_operand" "rmn")))]
  ""
  "quod %2,%0")

(define_insn "divhi3"
  [(set (match_operand:HI 0 "general_operand" "=g")
	(div:HI (match_operand:HI 1 "general_operand" "0")
		(match_operand:HI 2 "general_operand" "g")))]
  ""
  "quow %2,%0")

(define_insn "divqi3"
  [(set (match_operand:QI 0 "general_operand" "=g")
	(div:QI (match_operand:QI 1 "general_operand" "0")
		(match_operand:QI 2 "general_operand" "g")))]
  ""
  "quob %2,%0")

(define_insn "udivsi3"
  [(set (match_operand:SI 0 "register_operand" "=r")
	(udiv:SI (subreg:SI (match_operand:DI 1 "reg_or_mem_operand" "0") 0)
		 (match_operand:SI 2 "general_operand" "rmn")))]
  ""
  "*
{
  operands[1] = gen_rtx (REG, SImode, REGNO (operands[0]) + 1);
  return \"deid %2,%0\;movd %1,%0\";
}")

(define_insn "udivhi3"
  [(set (match_operand:HI 0 "register_operand" "=r")
	(udiv:HI (subreg:HI (match_operand:DI 1 "reg_or_mem_operand" "0") 0)
		 (match_operand:HI 2 "general_operand" "g")))]
  ""
  "*
{
  operands[1] = gen_rtx (REG, HImode, REGNO (operands[0]) + 1);
  return \"deiw %2,%0\;movw %1,%0\";
}")

(define_insn "udivqi3"
  [(set (match_operand:QI 0 "register_operand" "=r")
	(udiv:QI (subreg:QI (match_operand:DI 1 "reg_or_mem_operand" "0") 0)
		 (match_operand:QI 2 "general_operand" "g")))]
  ""
  "*
{
  operands[1] = gen_rtx (REG, QImode, REGNO (operands[0]) + 1);
  return \"deib %2,%0\;movb %1,%0\";
}")

;; Remainder instructions.

(define_insn "modsi3"
  [(set (match_operand:SI 0 "general_operand" "=g")
	(mod:SI (match_operand:SI 1 "general_operand" "0")
		(match_operand:SI 2 "general_operand" "rmn")))]
  ""
  "remd %2,%0")

(define_insn "modhi3"
  [(set (match_operand:HI 0 "general_operand" "=g")
	(mod:HI (match_operand:HI 1 "general_operand" "0")
		(match_operand:HI 2 "general_operand" "g")))]
  ""
  "remw %2,%0")

(define_insn "modqi3"
  [(set (match_operand:QI 0 "general_operand" "=g")
	(mod:QI (match_operand:QI 1 "general_operand" "0")
		(match_operand:QI 2 "general_operand" "g")))]
  ""
  "remb %2,%0")

(define_insn "umodsi3"
  [(set (match_operand:SI 0 "register_operand" "=r")
	(umod:SI (subreg:SI (match_operand:DI 1 "reg_or_mem_operand" "0") 0)
		 (match_operand:SI 2 "general_operand" "rmn")))]
  ""
  "deid %2,%0")

(define_insn "umodhi3"
  [(set (match_operand:HI 0 "register_operand" "=r")
	(umod:HI (subreg:HI (match_operand:DI 1 "reg_or_mem_operand" "0") 0)
		 (match_operand:HI 2 "general_operand" "g")))]
  ""
  "deiw %2,%0")

(define_insn "umodqi3"
  [(set (match_operand:QI 0 "register_operand" "=r")
	(umod:QI (subreg:QI (match_operand:DI 1 "reg_or_mem_operand" "0") 0)
		 (match_operand:QI 2 "general_operand" "g")))]
  ""
  "deib %2,%0")

; This isn't be usable in its current form.
;(define_insn "udivmoddisi4"
;  [(set (subreg:SI (match_operand:DI 0 "general_operand" "=r") 1)
;	(udiv:SI (match_operand:DI 1 "general_operand" "0")
;		 (match_operand:SI 2 "general_operand" "rmn")))
;   (set (subreg:SI (match_dup 0) 0)
;	(umod:SI (match_dup 1) (match_dup 2)))]
;  ""
;  "deid %2,%0")

;;- Logical Instructions: AND

(define_insn "andsi3"
  [(set (match_operand:SI 0 "general_operand" "=g")
	(and:SI (match_operand:SI 1 "general_operand" "%0")
		(match_operand:SI 2 "general_operand" "rmn")))]
  ""
  "*
{
  if (GET_CODE (operands[2]) == CONST_INT)
    {
      if ((INTVAL (operands[2]) | 0xff) == 0xffffffff)
	{
	  if (INTVAL (operands[2]) == 0xffffff00)
	    return \"movqb %$0,%0\";
	  else
	    {
	      operands[2] = GEN_INT (INTVAL (operands[2]) & 0xff);
	      return \"andb %2,%0\";
	    }
	}
      if ((INTVAL (operands[2]) | 0xffff) == 0xffffffff)
        {
	  if (INTVAL (operands[2]) == 0xffff0000)
	    return \"movqw %$0,%0\";
	  else
	    {
	      operands[2] = GEN_INT (INTVAL (operands[2]) & 0xffff);
	      return \"andw %2,%0\";
	    }
	}
    }
  return \"andd %2,%0\";
}")

(define_insn "andhi3"
  [(set (match_operand:HI 0 "general_operand" "=g")
	(and:HI (match_operand:HI 1 "general_operand" "%0")
		(match_operand:HI 2 "general_operand" "g")))]
  ""
  "*
{
  if (GET_CODE (operands[2]) == CONST_INT
      && (INTVAL (operands[2]) | 0xff) == 0xffffffff)
    {
      if (INTVAL (operands[2]) == 0xffffff00)
	return \"movqb %$0,%0\";
      else
	{
	  operands[2] = GEN_INT (INTVAL (operands[2]) & 0xff);
	  return \"andb %2,%0\";
	}
    }
  return \"andw %2,%0\";
}")

(define_insn "andqi3"
  [(set (match_operand:QI 0 "general_operand" "=g")
	(and:QI (match_operand:QI 1 "general_operand" "%0")
		(match_operand:QI 2 "general_operand" "g")))]
  ""
  "andb %2,%0")

(define_insn ""
  [(set (match_operand:SI 0 "general_operand" "=g")
	(and:SI (not:SI (match_operand:SI 1 "general_operand" "rmn"))
		(match_operand:SI 2 "general_operand" "0")))]
  ""
  "bicd %1,%0")

(define_insn ""
  [(set (match_operand:HI 0 "general_operand" "=g")
	(and:HI (not:HI (match_operand:HI 1 "general_operand" "g"))
		(match_operand:HI 2 "general_operand" "0")))]
  ""
  "bicw %1,%0")

(define_insn ""
  [(set (match_operand:QI 0 "general_operand" "=g")
	(and:QI (not:QI (match_operand:QI 1 "general_operand" "g"))
		(match_operand:QI 2 "general_operand" "0")))]
  ""
  "bicb %1,%0")

;;- Bit set instructions.

(define_insn "iorsi3"
  [(set (match_operand:SI 0 "general_operand" "=g")
	(ior:SI (match_operand:SI 1 "general_operand" "%0")
		(match_operand:SI 2 "general_operand" "rmn")))]
  ""
  "*
{
  if (GET_CODE (operands[2]) == CONST_INT) {
    if ((INTVAL (operands[2]) & 0xffffff00) == 0)
      return \"orb %2,%0\";
    if ((INTVAL (operands[2]) & 0xffff0000) == 0)
      return \"orw %2,%0\";
  }
  return \"ord %2,%0\";
}")

(define_insn "iorhi3"
  [(set (match_operand:HI 0 "general_operand" "=g")
	(ior:HI (match_operand:HI 1 "general_operand" "%0")
		(match_operand:HI 2 "general_operand" "g")))]
  ""
  "*
{
  if (GET_CODE(operands[2]) == CONST_INT &&
      (INTVAL(operands[2]) & 0xffffff00) == 0)
    return \"orb %2,%0\";
  return \"orw %2,%0\";
}")

(define_insn "iorqi3"
  [(set (match_operand:QI 0 "general_operand" "=g")
	(ior:QI (match_operand:QI 1 "general_operand" "%0")
		(match_operand:QI 2 "general_operand" "g")))]
  ""
  "orb %2,%0")

;;- xor instructions.

(define_insn "xorsi3"
  [(set (match_operand:SI 0 "general_operand" "=g")
	(xor:SI (match_operand:SI 1 "general_operand" "%0")
		(match_operand:SI 2 "general_operand" "rmn")))]
  ""
  "*
{
  if (GET_CODE (operands[2]) == CONST_INT) {
    if ((INTVAL (operands[2]) & 0xffffff00) == 0)
      return \"xorb %2,%0\";
    if ((INTVAL (operands[2]) & 0xffff0000) == 0)
      return \"xorw %2,%0\";
  }
  return \"xord %2,%0\";
}")

(define_insn "xorhi3"
  [(set (match_operand:HI 0 "general_operand" "=g")
	(xor:HI (match_operand:HI 1 "general_operand" "%0")
		(match_operand:HI 2 "general_operand" "g")))]
  ""
  "*
{
  if (GET_CODE(operands[2]) == CONST_INT &&
      (INTVAL(operands[2]) & 0xffffff00) == 0)
    return \"xorb %2,%0\";
  return \"xorw %2,%0\";
}")

(define_insn "xorqi3"
  [(set (match_operand:QI 0 "general_operand" "=g")
	(xor:QI (match_operand:QI 1 "general_operand" "%0")
		(match_operand:QI 2 "general_operand" "g")))]
  ""
  "xorb %2,%0")

(define_insn "negdf2"
  [(set (match_operand:DF 0 "general_operand" "=fm<")
	(neg:DF (match_operand:DF 1 "general_operand" "fmF")))]
  "TARGET_32081"
  "negl %1,%0")

(define_insn "negsf2"
  [(set (match_operand:SF 0 "general_operand" "=fm<")
	(neg:SF (match_operand:SF 1 "general_operand" "fmF")))]
  "TARGET_32081"
  "negf %1,%0")

(define_insn "negdi2"
  [(set (match_operand:DI 0 "general_operand" "=ro")
	(neg:DI (match_operand:DI 1 "general_operand" "ro")))]
  ""
  "*
{
  rtx low[2], high[2], xops[4];
  split_di (operands, 2, low, high);
  xops[0] = low[0];
  xops[1] = high[0];
  xops[2] = low[1];
  xops[3] = high[1];

  if (rtx_equal_p (operands[0], operands[1]))
    {
      output_asm_insn (\"negd %3,%1\", xops);
      output_asm_insn (\"negd %2,%0\", xops);
      output_asm_insn (\"subcd %$0,%1\", xops);
    }
  else
    {
      output_asm_insn (\"negd %2,%0\", xops);
      output_asm_insn (\"movqd %$0,%1\", xops);
      output_asm_insn (\"subcd %3,%1\", xops);
    }
  return \"\"; 
}")

(define_insn "negsi2"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(neg:SI (match_operand:SI 1 "general_operand" "rmn")))]
  ""
  "negd %1,%0")

(define_insn "neghi2"
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(neg:HI (match_operand:HI 1 "general_operand" "g")))]
  ""
  "negw %1,%0")

(define_insn "negqi2"
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(neg:QI (match_operand:QI 1 "general_operand" "g")))]
  ""
  "negb %1,%0")

(define_insn "one_cmplsi2"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(not:SI (match_operand:SI 1 "general_operand" "rmn")))]
  ""
  "comd %1,%0")

(define_insn "one_cmplhi2"
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(not:HI (match_operand:HI 1 "general_operand" "g")))]
  ""
  "comw %1,%0")

(define_insn "one_cmplqi2"
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(not:QI (match_operand:QI 1 "general_operand" "g")))]
  ""
  "comb %1,%0")

;; arithmetic left and right shift operations
;; on the 32532 we will always use lshd for arithmetic left shifts,
;; because it is three times faster.  Broken programs which
;; use negative shift counts are probably broken differently
;; than elsewhere.

;; alternative 0 never matches on the 32532
(define_insn "ashlsi3"
  [(set (match_operand:SI 0 "general_operand" "=g,g")
	(ashift:SI (match_operand:SI 1 "general_operand" "r,0")
		   (match_operand:SI 2 "general_operand" "I,rmn")))]
  ""
  "*
{ if (TARGET_32532)
    return \"lshd %2,%0\";
  else
    return output_shift_insn (operands);
}")

(define_insn "ashlhi3"
  [(set (match_operand:HI 0 "general_operand" "=g")
	(ashift:HI (match_operand:HI 1 "general_operand" "0")
		   (match_operand:SI 2 "general_operand" "rmn")))]
  ""
  "*
{ if (GET_CODE (operands[2]) == CONST_INT)
    {
      if (INTVAL (operands[2]) == 1)
	return \"addw %0,%0\";
      else if (! TARGET_32532 && INTVAL (operands[2]) == 2)
	return \"addw %0,%0\;addw %0,%0\";
    }
  if (TARGET_32532)
    return \"lshw %2,%0\";
  else
    return \"ashw %2,%0\";
}")

(define_insn "ashlqi3"
  [(set (match_operand:QI 0 "general_operand" "=g")
	(ashift:QI (match_operand:QI 1 "general_operand" "0")
		   (match_operand:SI 2 "general_operand" "rmn")))]
  ""
  "*
{ if (GET_CODE (operands[2]) == CONST_INT)
    {
      if (INTVAL (operands[2]) == 1)
	return \"addb %0,%0\";
      else if (! TARGET_32532 && INTVAL (operands[2]) == 2)
	return \"addb %0,%0\;addb %0,%0\";
    }
  if (TARGET_32532)
    return \"lshb %2,%0\";
  else
    return \"ashb %2,%0\";
}")

;; Arithmetic right shift on the 32k works by negating the shift count.
(define_expand "ashrsi3"
  [(set (match_operand:SI 0 "general_operand" "=g")
	(ashiftrt:SI (match_operand:SI 1 "general_operand" "g")
		     (match_operand:SI 2 "general_operand" "g")))]
  ""
  "
{
  if (GET_CODE (operands[2]) != CONST_INT)
    operands[2] = gen_rtx (NEG, SImode, negate_rtx (SImode, operands[2]));
}")

(define_insn ""
  [(set (match_operand:SI 0 "general_operand" "=g")
	(ashiftrt:SI (match_operand:SI 1 "general_operand" "0")
		     (match_operand:SI 2 "immediate_operand" "i")))]
  ""
  "ashd %$%n2,%0")

(define_insn ""
  [(set (match_operand:SI 0 "general_operand" "=g")
	(ashiftrt:SI (match_operand:SI 1 "general_operand" "0")
		     (neg:SI (match_operand:SI 2 "general_operand" "r"))))]
  ""
  "ashd %2,%0")

(define_expand "ashrhi3"
  [(set (match_operand:HI 0 "general_operand" "=g")
	(ashiftrt:HI (match_operand:HI 1 "general_operand" "g")
		     (match_operand:SI 2 "general_operand" "g")))]
  ""
  "
{
  if (GET_CODE (operands[2]) != CONST_INT)
    operands[2] = gen_rtx (NEG, SImode, negate_rtx (SImode, operands[2]));
}")

(define_insn ""
  [(set (match_operand:HI 0 "general_operand" "=g")
	(ashiftrt:HI (match_operand:HI 1 "general_operand" "0")
		     (match_operand:SI 2 "immediate_operand" "i")))]
  ""
  "ashw %$%n2,%0")

(define_insn ""
  [(set (match_operand:HI 0 "general_operand" "=g")
	(ashiftrt:HI (match_operand:HI 1 "general_operand" "0")
		     (neg:SI (match_operand:SI 2 "general_operand" "r"))))]
  ""
  "ashw %2,%0")

(define_expand "ashrqi3"
  [(set (match_operand:QI 0 "general_operand" "=g")
	(ashiftrt:QI (match_operand:QI 1 "general_operand" "g")
		     (match_operand:SI 2 "general_operand" "g")))]
  ""
  "
{
  if (GET_CODE (operands[2]) != CONST_INT)
    operands[2] = gen_rtx (NEG, SImode, negate_rtx (SImode, operands[2]));
}")

(define_insn ""
  [(set (match_operand:QI 0 "general_operand" "=g")
	(ashiftrt:QI (match_operand:QI 1 "general_operand" "0")
		     (match_operand:SI 2 "immediate_operand" "i")))]
  ""
  "ashb %$%n2,%0")

(define_insn ""
  [(set (match_operand:QI 0 "general_operand" "=g")
	(ashiftrt:QI (match_operand:QI 1 "general_operand" "0")
		     (neg:SI (match_operand:SI 2 "general_operand" "r"))))]
  ""
  "ashb %2,%0")

;; logical shift instructions

;; Logical right shift on the 32k works by negating the shift count.
(define_expand "lshrsi3"
  [(set (match_operand:SI 0 "general_operand" "=g")
	(lshiftrt:SI (match_operand:SI 1 "general_operand" "g")
		     (match_operand:SI 2 "general_operand" "g")))]
  ""
  "
{
  if (GET_CODE (operands[2]) != CONST_INT)
    operands[2] = gen_rtx (NEG, SImode, negate_rtx (SImode, operands[2]));
}")

(define_insn ""
  [(set (match_operand:SI 0 "general_operand" "=g")
	(lshiftrt:SI (match_operand:SI 1 "general_operand" "0")
		     (match_operand:SI 2 "immediate_operand" "i")))]
  ""
  "lshd %$%n2,%0")

(define_insn ""
  [(set (match_operand:SI 0 "general_operand" "=g")
	(lshiftrt:SI (match_operand:SI 1 "general_operand" "0")
		     (neg:SI (match_operand:SI 2 "general_operand" "r"))))]
  ""
  "lshd %2,%0")

(define_expand "lshrhi3"
  [(set (match_operand:HI 0 "general_operand" "=g")
	(lshiftrt:HI (match_operand:HI 1 "general_operand" "g")
		     (match_operand:SI 2 "general_operand" "g")))]
  ""
  "
{
  if (GET_CODE (operands[2]) != CONST_INT)
    operands[2] = gen_rtx (NEG, SImode, negate_rtx (SImode, operands[2]));
}")

(define_insn ""
  [(set (match_operand:HI 0 "general_operand" "=g")
	(lshiftrt:HI (match_operand:HI 1 "general_operand" "0")
		     (match_operand:SI 2 "immediate_operand" "i")))]
  ""
  "lshw %$%n2,%0")

(define_insn ""
  [(set (match_operand:HI 0 "general_operand" "=g")
	(lshiftrt:HI (match_operand:HI 1 "general_operand" "0")
		     (neg:SI (match_operand:SI 2 "general_operand" "r"))))]
  ""
  "lshw %2,%0")

(define_expand "lshrqi3"
  [(set (match_operand:QI 0 "general_operand" "=g")
	(lshiftrt:QI (match_operand:QI 1 "general_operand" "g")
		     (match_operand:SI 2 "general_operand" "g")))]
  ""
  "
{
  if (GET_CODE (operands[2]) != CONST_INT)
    operands[2] = gen_rtx (NEG, SImode, negate_rtx (SImode, operands[2]));
}")

(define_insn ""
  [(set (match_operand:QI 0 "general_operand" "=g")
	(lshiftrt:QI (match_operand:QI 1 "general_operand" "0")
		     (match_operand:SI 2 "immediate_operand" "i")))]
  ""
  "lshb %$%n2,%0")

(define_insn ""
  [(set (match_operand:QI 0 "general_operand" "=g")
	(lshiftrt:QI (match_operand:QI 1 "general_operand" "0")
		     (neg:SI (match_operand:SI 2 "general_operand" "r"))))]
  ""
  "lshb %2,%0")

;; Rotate instructions

(define_insn "rotlsi3"
  [(set (match_operand:SI 0 "general_operand" "=g")
	(rotate:SI (match_operand:SI 1 "general_operand" "0")
		   (match_operand:SI 2 "general_operand" "rmn")))]
  ""
  "rotd %2,%0")

(define_insn "rotlhi3"
  [(set (match_operand:HI 0 "general_operand" "=g")
	(rotate:HI (match_operand:HI 1 "general_operand" "0")
		   (match_operand:SI 2 "general_operand" "rmn")))]
  ""
  "rotw %2,%0")

(define_insn "rotlqi3"
  [(set (match_operand:QI 0 "general_operand" "=g")
	(rotate:QI (match_operand:QI 1 "general_operand" "0")
		   (match_operand:SI 2 "general_operand" "rmn")))]
  ""
  "rotb %2,%0")

;; Right rotate on the 32k works by negating the shift count.
(define_expand "rotrsi3"
  [(set (match_operand:SI 0 "general_operand" "=g")
	(rotatert:SI (match_operand:SI 1 "general_operand" "g")
		     (match_operand:SI 2 "general_operand" "g")))]
  ""
  "
{
  if (GET_CODE (operands[2]) != CONST_INT)
    operands[2] = gen_rtx (NEG, SImode, negate_rtx (SImode, operands[2]));
}")

(define_insn ""
  [(set (match_operand:SI 0 "general_operand" "=g")
	(rotatert:SI (match_operand:SI 1 "general_operand" "0")
		     (match_operand:SI 2 "immediate_operand" "i")))]
  ""
  "rotd %$%n2,%0")

(define_insn ""
  [(set (match_operand:SI 0 "general_operand" "=g")
	(rotatert:SI (match_operand:SI 1 "general_operand" "0")
		     (neg:SI (match_operand:SI 2 "general_operand" "r"))))]
  ""
  "rotd %2,%0")

(define_expand "rotrhi3"
  [(set (match_operand:HI 0 "general_operand" "=g")
	(rotatert:HI (match_operand:HI 1 "general_operand" "g")
		     (match_operand:SI 2 "general_operand" "g")))]
  ""
  "
{
  if (GET_CODE (operands[2]) != CONST_INT)
    operands[2] = gen_rtx (NEG, SImode, negate_rtx (SImode, operands[2]));
}")

(define_insn ""
  [(set (match_operand:HI 0 "general_operand" "=g")
	(rotatert:HI (match_operand:HI 1 "general_operand" "0")
		     (match_operand:SI 2 "immediate_operand" "i")))]
  ""
  "rotw %$%n2,%0")

(define_insn ""
  [(set (match_operand:HI 0 "general_operand" "=g")
	(rotatert:HI (match_operand:HI 1 "general_operand" "0")
		     (neg:SI (match_operand:SI 2 "general_operand" "r"))))]
  ""
  "rotw %2,%0")

(define_expand "rotrqi3"
  [(set (match_operand:QI 0 "general_operand" "=g")
	(rotatert:QI (match_operand:QI 1 "general_operand" "g")
		     (match_operand:SI 2 "general_operand" "g")))]
  ""
  "
{
  if (GET_CODE (operands[2]) != CONST_INT)
    operands[2] = gen_rtx (NEG, SImode, negate_rtx (SImode, operands[2]));
}")

(define_insn ""
  [(set (match_operand:QI 0 "general_operand" "=g")
	(rotatert:QI (match_operand:QI 1 "general_operand" "0")
		     (match_operand:SI 2 "immediate_operand" "i")))]
  ""
  "rotb %$%n2,%0")

(define_insn ""
  [(set (match_operand:QI 0 "general_operand" "=g")
	(rotatert:QI (match_operand:QI 1 "general_operand" "0")
		     (neg:SI (match_operand:SI 2 "general_operand" "r"))))]
  ""
  "rotb %2,%0")

;;- load or push effective address 
;; These come after the move, add, and multiply patterns
;; because we don't want pushl $1 turned into pushad 1.

(define_insn ""
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(match_operand:QI 1 "address_operand" "p"))]
  ""
  "*
{
  if (REG_P (operands[0])
      && GET_CODE (operands[1]) == MULT
      && GET_CODE (XEXP (operands[1], 1)) == CONST_INT
      && (INTVAL (XEXP (operands[1], 1)) == 2
	  || INTVAL (XEXP (operands[1], 1)) == 4))
    {
      rtx xoperands[3];
      xoperands[0] = operands[0];
      xoperands[1] = XEXP (operands[1], 0);
      xoperands[2] = GEN_INT (INTVAL (XEXP (operands[1], 1)) >> 1);
      return output_shift_insn (xoperands);
    }
  return \"addr %a1,%0\";
}")

;;; Index insns.  These are about the same speed as multiply-add counterparts.
;;; but slower then using power-of-2 shifts if we can use them
;
;(define_insn ""
;  [(set (match_operand:SI 0 "register_operand" "=r")
;	(plus:SI (match_operand:SI 1 "general_operand" "rmn")
;		 (mult:SI (match_operand:SI 2 "register_operand" "0")
;			  (plus:SI (match_operand:SI 3 "general_operand" "rmn") (const_int 1)))))]
;  "GET_CODE (operands[3]) != CONST_INT || INTVAL (operands[3]) > 8"
;  "indexd %0,%3,%1")
;
;(define_insn ""
;  [(set (match_operand:SI 0 "register_operand" "=r")
;	(plus:SI (mult:SI (match_operand:SI 1 "register_operand" "0")
;			  (plus:SI (match_operand:SI 2 "general_operand" "rmn") (const_int 1)))
;		 (match_operand:SI 3 "general_operand" "rmn")))]
;  "GET_CODE (operands[2]) != CONST_INT || INTVAL (operands[2]) > 8"
;  "indexd %0,%2,%3")

;; Set, Clear, and Invert bit

(define_insn ""
  [(set (zero_extract:SI (match_operand:SI 0 "general_operand" "+g")
			 (const_int 1)
			 (match_operand:SI 1 "general_operand" "rmn"))
	(const_int 1))]
  ""
  "sbitd %1,%0")

(define_insn ""
  [(set (zero_extract:SI (match_operand:SI 0 "general_operand" "+g")
			 (const_int 1)
			 (match_operand:SI 1 "general_operand" "rmn"))
	(const_int 0))]
  ""
  "cbitd %1,%0")

(define_insn ""
  [(set (match_operand:SI 0 "general_operand" "+g")
	(xor:SI (ashift:SI (const_int 1)
			   (match_operand:SI 1 "general_operand" "rmn"))
		(match_dup 0)))]
  ""
  "ibitd %1,%0")

(define_insn ""
  [(set (match_operand:QI 0 "general_operand" "=g")
	(xor:QI (subreg:QI
		 (ashift:SI (const_int 1)
			    (match_operand:QI 1 "general_operand" "rmn")) 0)
		(match_dup 0)))]
  ""
  "ibitb %1,%0")

;; Recognize jbs and jbc instructions.

(define_insn ""
  [(set (cc0)
	(zero_extract (match_operand:SI 0 "general_operand" "rm")
		      (const_int 1)
		      (match_operand:SI 1 "general_operand" "g")))]
  ""
  "*
{ cc_status.flags = CC_Z_IN_F;
  return \"tbitd %1,%0\";
}")

;; extract(base, width, offset)
;; Signed bitfield extraction is not supported in hardware on the
;; NS 32032.  It is therefore better to let GCC figure out a
;; good strategy for generating the proper instruction sequence
;; and represent it as rtl.

;; Optimize the case of extracting a byte or word from a register.
;; Otherwise we must load a register with the offset of the
;; chunk we want, and perform an extract insn (each of which
;; is very expensive).  Since we use the stack to do our bit-twiddling
;; we cannot use it for a destination.  Perhaps things are fast
;; enough on the 32532 that such hacks are not needed.

(define_insn ""
  [(set (match_operand:SI 0 "general_operand" "=ro")
	(zero_extract:SI (match_operand:SI 1 "register_operand" "r")
			 (match_operand:SI 2 "const_int_operand" "i")
			 (match_operand:SI 3 "const_int_operand" "i")))]
  "(INTVAL (operands[2]) == 8 || INTVAL (operands[2]) == 16)
   && (INTVAL (operands[3]) == 8 || INTVAL (operands[3]) == 16 || INTVAL (operands[3]) == 24)"
  "*
{
  output_asm_insn (\"movd %1,tos\", operands);
  if (INTVAL (operands[2]) == 16)
    {
      if (INTVAL (operands[3]) == 8)
	output_asm_insn (\"movzwd 1(sp),%0\", operands);
      else
	output_asm_insn (\"movzwd 2(sp),%0\", operands);
    }
  else
    {
      if (INTVAL (operands[3]) == 8)
	output_asm_insn (\"movzbd 1(sp),%0\", operands);
      else if (INTVAL (operands[3]) == 16)
	output_asm_insn (\"movzbd 2(sp),%0\", operands);
      else
	output_asm_insn (\"movzbd 3(sp),%0\", operands);
    }
  if (TARGET_32532 || TARGET_32332)
    return \"cmpqd %$0,tos\";
  else
    return \"adjspb %$-4\";
}")

;; The exts/ext instructions have the problem that they always access
;; 32 bits even if the bitfield is smaller. For example the instruction
;; 	extsd 7(r1),r0,2,5
;; would read not only at address 7(r1) but also at 8(r1) to 10(r1).
;; If these addresses are in a different (unmapped) page a memory fault
;; is the result.
;;
;; Timing considerations:
;;	movd	0(r1),r0	3 bytes
;;	lshd	-26,r0		4
;;	andd	0x1f,r0		5
;; takes about 13 cycles on the 532 while
;;	extsd	7(r1),r0,2,5	5 bytes
;; takes about 21 cycles.
;;
;; The inss/ins instructions suffer from the same problem.
;;
;; A machine specific option (-mbitfield/-mnobitfield) is used
;; to allow/disallow the use of these instructions.

(define_insn ""
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(zero_extract:SI (match_operand:SI 1 "register_operand" "g")
			 (match_operand:SI 2 "const_int_operand" "i")
			 (match_operand:SI 3 "general_operand" "rK")))]
  "TARGET_BITFIELD"
  "*
{ if (GET_CODE (operands[3]) == CONST_INT)
    return \"extsd %1,%0,%3,%2\";
  else return \"extd %3,%1,%0,%2\";
}")

(define_insn "extzv"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(zero_extract:SI (match_operand:QI 1 "general_operand" "g")
			 (match_operand:SI 2 "const_int_operand" "i")
			 (match_operand:SI 3 "general_operand" "rK")))]
  "TARGET_BITFIELD"
  "*
{ if (GET_CODE (operands[3]) == CONST_INT)
    return \"extsd %1,%0,%3,%2\";
  else return \"extd %3,%1,%0,%2\";
}")

(define_insn ""
  [(set (zero_extract:SI (match_operand:SI 0 "memory_operand" "+o")
			 (match_operand:SI 1 "const_int_operand" "i")
			 (match_operand:SI 2 "general_operand" "rn"))
	(match_operand:SI 3 "general_operand" "rm"))]
  "TARGET_BITFIELD"
  "*
{ if (GET_CODE (operands[2]) == CONST_INT)
    {
      if (INTVAL (operands[2]) >= 8)
	{
	  operands[0] = adj_offsettable_operand (operands[0],
					        INTVAL (operands[2]) / 8);
          operands[2] = GEN_INT (INTVAL (operands[2]) % 8);
	}
      if (INTVAL (operands[1]) <= 8)
        return \"inssb %3,%0,%2,%1\";
      else if (INTVAL (operands[1]) <= 16)
	return \"inssw %3,%0,%2,%1\";
      else
	return \"inssd %3,%0,%2,%1\";
    }
  return \"insd %2,%3,%0,%1\";
}")

(define_insn ""
  [(set (zero_extract:SI (match_operand:SI 0 "register_operand" "+r")
			 (match_operand:SI 1 "const_int_operand" "i")
			 (match_operand:SI 2 "general_operand" "rK"))
	(match_operand:SI 3 "general_operand" "rm"))]
  "TARGET_BITFIELD"
  "*
{ if (GET_CODE (operands[2]) == CONST_INT)
    if (INTVAL (operands[1]) <= 8)
      return \"inssb %3,%0,%2,%1\";
    else if (INTVAL (operands[1]) <= 16)
      return \"inssw %3,%0,%2,%1\";
    else
      return \"inssd %3,%0,%2,%1\";
  return \"insd %2,%3,%0,%1\";
}")

(define_insn "insv"
  [(set (zero_extract:SI (match_operand:QI 0 "general_operand" "+g")
			 (match_operand:SI 1 "const_int_operand" "i")
			 (match_operand:SI 2 "general_operand" "rK"))
	(match_operand:SI 3 "general_operand" "rm"))]
  "TARGET_BITFIELD"
  "*
{ if (GET_CODE (operands[2]) == CONST_INT)
    if (INTVAL (operands[1]) <= 8)
      return \"inssb %3,%0,%2,%1\";
    else if (INTVAL (operands[1]) <= 16)
      return \"inssw %3,%0,%2,%1\";
    else
      return \"inssd %3,%0,%2,%1\";
  return \"insd %2,%3,%0,%1\";
}")


(define_insn "jump"
  [(set (pc)
	(label_ref (match_operand 0 "" "")))]
  ""
  "br %l0")

(define_insn "beq"
  [(set (pc)
	(if_then_else (eq (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "*
{ if (cc_prev_status.flags & CC_Z_IN_F)
    return \"bfc %l0\";
  else if (cc_prev_status.flags & CC_Z_IN_NOT_F)
    return \"bfs %l0\";
  else return \"beq %l0\";
}")

(define_insn "bne"
  [(set (pc)
	(if_then_else (ne (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "*
{ if (cc_prev_status.flags & CC_Z_IN_F)
    return \"bfs %l0\";
  else if (cc_prev_status.flags & CC_Z_IN_NOT_F)
    return \"bfc %l0\";
  else return \"bne %l0\";
}")

(define_insn "bgt"
  [(set (pc)
	(if_then_else (gt (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "bgt %l0")

(define_insn "bgtu"
  [(set (pc)
	(if_then_else (gtu (cc0)
			   (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "bhi %l0")

(define_insn "blt"
  [(set (pc)
	(if_then_else (lt (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "blt %l0")

(define_insn "bltu"
  [(set (pc)
	(if_then_else (ltu (cc0)
			   (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "blo %l0")

(define_insn "bge"
  [(set (pc)
	(if_then_else (ge (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "bge %l0")

(define_insn "bgeu"
  [(set (pc)
	(if_then_else (geu (cc0)
			   (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "bhs %l0")

(define_insn "ble"
  [(set (pc)
	(if_then_else (le (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "ble %l0")

(define_insn "bleu"
  [(set (pc)
	(if_then_else (leu (cc0)
			   (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "bls %l0")

(define_insn ""
  [(set (pc)
	(if_then_else (eq (cc0)
			  (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
  "*
{ if (cc_prev_status.flags & CC_Z_IN_F)
    return \"bfs %l0\";
  else if (cc_prev_status.flags & CC_Z_IN_NOT_F)
    return \"bfc %l0\";
  else return \"bne %l0\";
}")

(define_insn ""
  [(set (pc)
	(if_then_else (ne (cc0)
			  (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
  "*
{ if (cc_prev_status.flags & CC_Z_IN_F)
    return \"bfc %l0\";
  else if (cc_prev_status.flags & CC_Z_IN_NOT_F)
    return \"bfs %l0\";
  else return \"beq %l0\";
}")

(define_insn ""
  [(set (pc)
	(if_then_else (gt (cc0)
			  (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
  "ble %l0")

(define_insn ""
  [(set (pc)
	(if_then_else (gtu (cc0)
			   (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
  "bls %l0")

(define_insn ""
  [(set (pc)
	(if_then_else (lt (cc0)
			  (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
  "bge %l0")

(define_insn ""
  [(set (pc)
	(if_then_else (ltu (cc0)
			   (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
  "bhs %l0")

(define_insn ""
  [(set (pc)
	(if_then_else (ge (cc0)
			  (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
  "blt %l0")

(define_insn ""
  [(set (pc)
	(if_then_else (geu (cc0)
			   (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
  "blo %l0")

(define_insn ""
  [(set (pc)
	(if_then_else (le (cc0)
			  (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
  "bgt %l0")

(define_insn ""
  [(set (pc)
	(if_then_else (leu (cc0)
			   (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
  "bhi %l0")

;; Subtract-and-jump and Add-and-jump insns.
;; These can actually be used for adding numbers in the range -8 to 7

(define_insn ""
  [(set (pc)
	(if_then_else
	 (ne (match_operand:SI 0 "general_operand" "+g")
	     (match_operand:SI 1 "const_int_operand" "i"))
	 (label_ref (match_operand 2 "" ""))
	 (pc)))
  (set (match_dup 0)
       (minus:SI (match_dup 0)
		 (match_dup 1)))]
  "INTVAL (operands[1]) > -8 && INTVAL (operands[1]) <= 8"
  "acbd %$%n1,%0,%l2")

(define_insn ""
  [(set (pc)
	(if_then_else
	 (ne (match_operand:SI 0 "general_operand" "+g")
	     (match_operand:SI 1 "const_int_operand" "i"))
	 (label_ref (match_operand 2 "" ""))
	 (pc)))
  (set (match_dup 0)
       (plus:SI (match_dup 0)
		(match_operand:SI 3 "const_int_operand" "i")))]
  "INTVAL (operands[1]) == - INTVAL (operands[3])
   && INTVAL (operands[3]) >= -8 && INTVAL (operands[3]) < 8"
  "acbd %3,%0,%l2")

(define_insn "call"
  [(call (match_operand:QI 0 "memory_operand" "m")
	 (match_operand:QI 1 "general_operand" "g"))]
  ""
  "*
{
#ifndef JSR_ALWAYS
  if (GET_CODE (operands[0]) == MEM)
    {
      rtx temp = XEXP (operands[0], 0);
      if (CONSTANT_ADDRESS_P (temp))
	{
#ifdef ENCORE_ASM
	  return \"bsr %?%0\";
#else
#ifdef CALL_MEMREF_IMPLICIT
	  operands[0] = temp;
	  return \"bsr %0\";
#else
#ifdef GNX_V3
	  return \"bsr %0\";
#else
	  return \"bsr %?%a0\";
#endif
#endif
#endif
	}
      if (GET_CODE (XEXP (operands[0], 0)) == REG)
#if defined (GNX_V3) || defined (CALL_MEMREF_IMPLICIT)
	return \"jsr %0\";
#else
        return \"jsr %a0\";
#endif
    }
#endif /* not JSR_ALWAYS */
  return \"jsr %0\";
}")

(define_insn "call_value"
  [(set (match_operand 0 "" "=rf")
	(call (match_operand:QI 1 "memory_operand" "m")
	      (match_operand:QI 2 "general_operand" "g")))]
  ""
  "*
{
#ifndef JSR_ALWAYS
  if (GET_CODE (operands[1]) == MEM)
    {
      rtx temp = XEXP (operands[1], 0);
      if (CONSTANT_ADDRESS_P (temp))
	{
#ifdef ENCORE_ASM
	  return \"bsr %?%1\";
#else
#ifdef CALL_MEMREF_IMPLICIT
	  operands[1] = temp;
	  return \"bsr %1\";
#else
#ifdef GNX_V3
	  return \"bsr %1\";
#else
	  return \"bsr %?%a1\";
#endif
#endif
#endif
	}
      if (GET_CODE (XEXP (operands[1], 0)) == REG)
#if defined (GNX_V3) || defined (CALL_MEMREF_IMPLICIT)
	return \"jsr %1\";
#else
        return \"jsr %a1\";
#endif
    }
#endif /* not JSR_ALWAYS */
  return \"jsr %1\";
}")

;; Call subroutine returning any type.

(define_expand "untyped_call"
  [(parallel [(call (match_operand 0 "" "")
		    (const_int 0))
	      (match_operand 1 "" "")
	      (match_operand 2 "" "")])]
  ""
  "
{
  int i;

  emit_call_insn (gen_call (operands[0], const0_rtx, NULL, const0_rtx));

  for (i = 0; i < XVECLEN (operands[2], 0); i++)
    {
      rtx set = XVECEXP (operands[2], 0, i);
      emit_move_insn (SET_DEST (set), SET_SRC (set));
    }

  /* The optimizer does not know that the call sets the function value
     registers we stored in the result block.  We avoid problems by
     claiming that all hard registers are used and clobbered at this
     point.  */
  emit_insn (gen_blockage ());

  DONE;
}")

;; UNSPEC_VOLATILE is considered to use and clobber all hard registers and
;; all of memory.  This blocks insns from being moved across this point.

(define_insn "blockage"
  [(unspec_volatile [(const_int 0)] 0)]
  ""
  "")

(define_insn "return"
  [(return)]
  "0"
  "ret 0")

(define_insn "abssf2"
  [(set (match_operand:SF 0 "general_operand" "=fm<")
	(abs:SF (match_operand:SF 1 "general_operand" "fmF")))]
  "TARGET_32081"
  "absf %1,%0")

(define_insn "absdf2"
  [(set (match_operand:DF 0 "general_operand" "=fm<")
	(abs:DF (match_operand:DF 1 "general_operand" "fmF")))]
  "TARGET_32081"
  "absl %1,%0")

(define_insn "abssi2"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(abs:SI (match_operand:SI 1 "general_operand" "rmn")))]
  ""
  "absd %1,%0")

(define_insn "abshi2"
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(abs:HI (match_operand:HI 1 "general_operand" "g")))]
  ""
  "absw %1,%0")

(define_insn "absqi2"
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(abs:QI (match_operand:QI 1 "general_operand" "g")))]
  ""
  "absb %1,%0")

(define_insn "nop"
  [(const_int 0)]
  ""
  "nop")

(define_insn "indirect_jump"
  [(set (pc) (match_operand:SI 0 "register_operand" "r"))]
  ""
  "jump %0")

(define_insn "tablejump"
  [(set (pc)
	(plus:SI (pc) (match_operand:SI 0 "general_operand" "g")))
   (use (label_ref (match_operand 1 "" "")))]
  ""
  "*
{
  ASM_OUTPUT_INTERNAL_LABEL (asm_out_file, \"LI\",
			     CODE_LABEL_NUMBER (operands[1]));
  return \"cased %0\";
}")

;; Scondi instructions
(define_insn "seq"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(eq:SI (cc0) (const_int 0)))]
  ""
  "*
{ if (cc_prev_status.flags & CC_Z_IN_F)
    return \"sfcd %0\";
  else if (cc_prev_status.flags & CC_Z_IN_NOT_F)
    return \"sfsd %0\";
  else return \"seqd %0\";
}")

(define_insn ""
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(eq:HI (cc0) (const_int 0)))]
  ""
  "*
{ if (cc_prev_status.flags & CC_Z_IN_F)
    return \"sfcw %0\";
  else if (cc_prev_status.flags & CC_Z_IN_NOT_F)
    return \"sfsw %0\";
  else return \"seqw %0\";
}")

(define_insn ""
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(eq:QI (cc0) (const_int 0)))]
  ""
  "*
{ if (cc_prev_status.flags & CC_Z_IN_F)
    return \"sfcb %0\";
  else if (cc_prev_status.flags & CC_Z_IN_NOT_F)
    return \"sfsb %0\";
  else return \"seqb %0\";
}")

(define_insn "sne"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(ne:SI (cc0) (const_int 0)))]
  ""
  "*
{ if (cc_prev_status.flags & CC_Z_IN_F)
    return \"sfsd %0\";
  else if (cc_prev_status.flags & CC_Z_IN_NOT_F)
    return \"sfcd %0\";
  else return \"sned %0\";
}")

(define_insn ""
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(ne:HI (cc0) (const_int 0)))]
  ""
  "*
{ if (cc_prev_status.flags & CC_Z_IN_F)
    return \"sfsw %0\";
  else if (cc_prev_status.flags & CC_Z_IN_NOT_F)
    return \"sfcw %0\";
  else return \"snew %0\";
}")

(define_insn ""
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(ne:QI (cc0) (const_int 0)))]
  ""
  "*
{ if (cc_prev_status.flags & CC_Z_IN_F)
    return \"sfsb %0\";
  else if (cc_prev_status.flags & CC_Z_IN_NOT_F)
    return \"sfcb %0\";
  else return \"sneb %0\";
}")

(define_insn "sgt"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(gt:SI (cc0) (const_int 0)))]
  ""
  "sgtd %0")

(define_insn ""
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(gt:HI (cc0) (const_int 0)))]
  ""
  "sgtw %0")

(define_insn ""
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(gt:QI (cc0) (const_int 0)))]
  ""
  "sgtb %0")

(define_insn "sgtu"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(gtu:SI (cc0) (const_int 0)))]
  ""
  "shid %0")

(define_insn ""
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(gtu:HI (cc0) (const_int 0)))]
  ""
  "shiw %0")

(define_insn ""
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(gtu:QI (cc0) (const_int 0)))]
  ""
  "shib %0")

(define_insn "slt"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(lt:SI (cc0) (const_int 0)))]
  ""
  "sltd %0")

(define_insn ""
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(lt:HI (cc0) (const_int 0)))]
  ""
  "sltw %0")

(define_insn ""
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(lt:QI (cc0) (const_int 0)))]
  ""
  "sltb %0")

(define_insn "sltu"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(ltu:SI (cc0) (const_int 0)))]
  ""
  "slod %0")

(define_insn ""
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(ltu:HI (cc0) (const_int 0)))]
  ""
  "slow %0")

(define_insn ""
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(ltu:QI (cc0) (const_int 0)))]
  ""
  "slob %0")

(define_insn "sge"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(ge:SI (cc0) (const_int 0)))]
  ""
  "sged %0")

(define_insn ""
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(ge:HI (cc0) (const_int 0)))]
  ""
  "sgew %0")

(define_insn ""
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(ge:QI (cc0) (const_int 0)))]
  ""
  "sgeb %0")

(define_insn "sgeu"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(geu:SI (cc0) (const_int 0)))]
  ""
  "shsd %0")  

(define_insn ""
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(geu:HI (cc0) (const_int 0)))]
  ""
  "shsw %0")  

(define_insn ""
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(geu:QI (cc0) (const_int 0)))]
  ""
  "shsb %0")  

(define_insn "sle"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(le:SI (cc0) (const_int 0)))]
  ""
  "sled %0")

(define_insn ""
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(le:HI (cc0) (const_int 0)))]
  ""
  "slew %0")

(define_insn ""
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(le:QI (cc0) (const_int 0)))]
  ""
  "sleb %0")

(define_insn "sleu"
  [(set (match_operand:SI 0 "general_operand" "=g<")
	(leu:SI (cc0) (const_int 0)))]
  ""
  "slsd %0")

(define_insn ""
  [(set (match_operand:HI 0 "general_operand" "=g<")
	(leu:HI (cc0) (const_int 0)))]
  ""
  "slsw %0")

(define_insn ""
  [(set (match_operand:QI 0 "general_operand" "=g<")
	(leu:QI (cc0) (const_int 0)))]
  ""
  "slsb %0")

;; ffs instructions

(define_insn ""
  [(set (match_operand:SI 0 "general_operand" "ro")
	(minus:SI 
		(plus:SI (ffs:SI (zero_extract:SI 
				(match_operand:SI 1 "general_operand" "g") 
				(minus:SI (const_int 32) (match_dup 0))
				(match_dup 0)))
			(match_dup 0)) 
		(const_int 1)))]
  ""
  "ffsd %1,%0; bfc 1f; addqd %$-1,%0; 1:")

(define_expand "ffssi2"
  [(set (match_operand:SI 0 "general_operand" "=g") (const_int 0))
   (set (match_dup 0)
	(minus:SI 
		(plus:SI (ffs:SI (zero_extract:SI 
				(match_operand:SI 1 "general_operand" "g") 
				(minus:SI (const_int 32) (match_dup 0))
				(match_dup 0)))
			(match_dup 0)) 
		(const_int 1)))
   (set (match_dup 0)
	(plus:SI (match_dup 0)
		 (const_int 1)))]
  ""
  "operands[1] = make_safe_from(operands[1], operands[0]);")

;; Speed up stack adjust followed by a HI fixedpoint push.

(define_peephole
  [(set (reg:SI 17) (plus:SI (reg:SI 17) (const_int -2)))
   (set (match_operand:HI 0 "push_operand" "=m")
	(match_operand:HI 1 "general_operand" "g"))]
  "! reg_mentioned_p (stack_pointer_rtx, operands[1])"
  "*
{
  if (GET_CODE (operands[1]) == CONST_INT)
	output_asm_insn (output_move_dconst (INTVAL (operands[1]), \"%$%1,tos\"),
			 operands);
  else
	output_asm_insn (\"movzwd %1,tos\", operands);
  return \"\";
}")

;; Speed up stack adjust followed by a zero_extend:HI(QI) fixedpoint push.

(define_peephole
  [(set (reg:SI 17) (plus:SI (reg:SI 17) (const_int -2)))
   (set (match_operand:HI 0 "push_operand" "=m")
	(zero_extend:HI (match_operand:QI 1 "general_operand" "g")))]
  "! reg_mentioned_p (stack_pointer_rtx, operands[1])"
  "*
{
  if (GET_CODE (operands[1]) == CONST_INT)
	output_asm_insn (output_move_dconst (INTVAL (operands[1]), \"%$%1,tos\"),
			 operands);
  else
	output_asm_insn (\"movzbd %1,tos\", operands);
  return \"\";
}")

;; Speed up stack adjust followed by a sign_extend:HI(QI) fixedpoint push.

(define_peephole
  [(set (reg:SI 17) (plus:SI (reg:SI 17) (const_int -2)))
   (set (match_operand:HI 0 "push_operand" "=m")
	(sign_extend:HI (match_operand:QI 1 "general_operand" "g")))]
  "! reg_mentioned_p (stack_pointer_rtx, operands[1])"
  "*
{
  if (GET_CODE (operands[1]) == CONST_INT)
	output_asm_insn (output_move_dconst (INTVAL (operands[1]), \"%$%1,tos\"),
			 operands);
  else
	output_asm_insn (\"movxbd %1,tos\", operands);
  return \"\";
}")

;; Speed up stack adjust followed by a QI fixedpoint push.

(define_peephole
  [(set (reg:SI 17) (plus:SI (reg:SI 17) (const_int -3)))
   (set (match_operand:QI 0 "push_operand" "=m")
	(match_operand:QI 1 "general_operand" "g"))]
  "! reg_mentioned_p (stack_pointer_rtx, operands[1])"
  "*
{
  if (GET_CODE (operands[1]) == CONST_INT)
	output_asm_insn (output_move_dconst (INTVAL (operands[1]), \"%$%1,tos\"),
			 operands);
  else
	output_asm_insn (\"movzbd %1,tos\", operands);
  return \"\";
}")

;; Speed up stack adjust followed by a SI fixedpoint push.

(define_peephole
  [(set (reg:SI 17) (plus:SI (reg:SI 17) (const_int 4)))
   (set (match_operand:SI 0 "push_operand" "=m")
	(match_operand:SI 1 "general_operand" "g"))]
  "! reg_mentioned_p (stack_pointer_rtx, operands[1])"
  "*
{
  if (GET_CODE (operands[1]) == CONST_INT)
	output_asm_insn (output_move_dconst (INTVAL (operands[1]), \"%$%1,0(sp)\"),
			 operands);
  else if (GET_CODE (operands[1]) != REG
	   && GET_CODE (operands[1]) != MEM
	   && address_operand (operands[1], SImode))
	output_asm_insn (\"addr %a1,0(sp)\", operands);
  else
	output_asm_insn (\"movd %1,0(sp)\", operands);
  return \"\";
}")

;; Speed up stack adjust followed by two fullword fixedpoint pushes.

(define_peephole
  [(set (reg:SI 17) (plus:SI (reg:SI 17) (const_int 8)))
   (set (match_operand:SI 0 "push_operand" "=m")
	(match_operand:SI 1 "general_operand" "g"))
   (set (match_operand:SI 2 "push_operand" "=m")
	(match_operand:SI 3 "general_operand" "g"))]
  "! reg_mentioned_p (stack_pointer_rtx, operands[1])
   && ! reg_mentioned_p (stack_pointer_rtx, operands[3])"
  "*
{
  if (GET_CODE (operands[1]) == CONST_INT)
	output_asm_insn (output_move_dconst (INTVAL (operands[1]), \"%$%1,4(sp)\"),
			 operands);
  else if (GET_CODE (operands[1]) != REG
	   && GET_CODE (operands[1]) != MEM
	   && address_operand (operands[1], SImode))
	output_asm_insn (\"addr %a1,4(sp)\", operands);
  else
	output_asm_insn (\"movd %1,4(sp)\", operands);

  if (GET_CODE (operands[3]) == CONST_INT)
	output_asm_insn (output_move_dconst (INTVAL (operands[3]), \"%$%3,0(sp)\"),
			 operands);
  else if (GET_CODE (operands[3]) != REG
	   && GET_CODE (operands[3]) != MEM
	   && address_operand (operands[3], SImode))
	output_asm_insn (\"addr %a3,0(sp)\", operands);
  else
	output_asm_insn (\"movd %3,0(sp)\", operands);
  return \"\";
}")
