;;- Machine description for GNU compiler, Clipper Version
;;   Copyright (C) 1987, 1988, 1991 Free Software Foundation, Inc.

;; Contributed by Holger Teutsch (holger@hotbso.rhein-main.de)

;; This file is part of GNU CC.

;; GNU CC is free software; you can redistribute it and/or modify
;; it under the terms of the GNU General Public License as published by
;; the Free Software Foundation; either version 2, or (at your option)
;; any later version.

;; GNU CC is distributed in the hope that it will be useful,
;; but WITHOUT ANY WARRANTY; without even the implied warranty of
;; MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
;; GNU General Public License for more details.

;; You should have received a copy of the GNU General Public License
;; along with GNU CC; see the file COPYING.  If not, write to
;; the Free Software Foundation, 675 Mass Ave, Cambridge, MA 02139, USA.


;;- Instruction patterns.  When multiple patterns apply,
;;- the first one in the file is chosen.
;;-
;;- See file "rtl.def" for documentation on define_insn, match_*, et. al.
;;-
;;- cpp macro #define NOTICE_UPDATE_CC in file tm.h handles condition code
;;- updates for most instructions.

;;
;; define attributes
;;
;; instruction type
;;
;; unknown is temporary in order to generate 'cc clobber' until attribute
;; assignment is consistent
;;
(define_attr "type" "load,store,arith,fp,branch,unknown"
 (const_string "unknown"))

;; condition code setting
;;
;; clobber	destroyed
;; unchanged
;; set1		set cc_status.value1, e.g. sub r0,r1
;; set2		set value1 and value2, e.g. mov r0,r1
;; change0	may be side effect, i.e. load mem,r0
;;
;; note: loadi and loadq are 'arith' instructions that set the condition codes
;;       mul,div,mod do NOT set the condition codes
;;
(define_attr "cc" "clobber,unchanged,set1,set2,change0"
 (cond [(eq_attr "type" "load")	(const_string "change0")
	(eq_attr "type" "store,branch") (const_string "unchanged")
	(eq_attr "type" "arith") (if_then_else (match_operand:SI 0 "" "")
				  (const_string "set1")
				  (const_string "clobber"))
	]
  (const_string "clobber")))

;;
;; clipper seems to be a tradional risc processor
;; we define a functional unit 'memory'
;;
(define_function_unit "memory" 1 1 (eq_attr "type" "load") 4 0)     


;; We don't want to allow a constant operand for test insns because
;; (set (cc0) (const_int foo)) has no mode information.  Such insns will
;; be folded while optimizing anyway.

(define_insn "tstsi"
  [(set (cc0)
	(match_operand:SI 0 "int_reg_operand" "r"))]
  ""
  "cmpq   $0,%0")

(define_insn "cmpsi"
  [(set (cc0)
	(compare (match_operand:SI 0 "nonimmediate_operand" "r,r,n")
		 (match_operand:SI 1 "nonmemory_operand" "r,n,r")))]
  ""
  "*
{
  int val;

  if (which_alternative == 0)
    return \"cmpw   %1,%0\";

  if (which_alternative == 1)
    {
      val = INTVAL (operands[1]);
      if (0 <= val && val < 16)
	return \"cmpq   %1,%0\";
      return \"cmpi   %1,%0\";
    }

  cc_status.flags |= CC_REVERSED;	/* immediate must be first */

  val = INTVAL (operands[0]);

  if (0 <= val && val < 16)
    return \"cmpq   %0,%1\";

  return \"cmpi   %0,%1\";
}")

(define_insn "cmpdf"
  [(set (cc0)
	(compare (match_operand:DF 0 "fp_reg_operand" "f")
		 (match_operand:DF 1 "fp_reg_operand" "f")))]
  ""
  "cmpd   %1,%0")

(define_insn "cmpsf"
  [(set (cc0)
	(compare (match_operand:SF 0 "fp_reg_operand" "f")
		 (match_operand:SF 1 "fp_reg_operand" "f")))]
  ""
  "cmps   %1,%0")


;;
;; double and single float move
;;
(define_expand "movdf"
  [(set (match_operand:DF 0 "general_operand" "")
	(match_operand:DF 1 "general_operand" ""))]
  ""
  "
{
  if (GET_CODE (operands[0]) == MEM)
    {
      if (GET_CODE (operands[1]) == CONST_DOUBLE)
	operands[1] = force_reg (DFmode,
				 force_const_mem (DFmode, operands[1]));
      else if (GET_CODE (operands[1]) != REG)
	operands[1] = force_reg (DFmode, operands[1]);
    }

  else if (GET_CODE (operands[1]) == CONST_DOUBLE)
    operands[1] = force_const_mem (DFmode, operands[1]);
}")

;;
;; provide two patterns with different predicates as we don't want combine
;; to recombine a mem -> mem move
;; 
(define_insn ""
  [(set (match_operand:DF 0 "register_operand" "=rf")
	(match_operand:DF 1 "nonimmediate_operand" "rfo"))]
  ""
  "*
{
#define FP_REG_P(X) (GET_CODE (X) == REG && REGNO (X) >= 16)

  if (FP_REG_P (operands[0]))
    {
      if (FP_REG_P (operands[1]))	/* f -> f */
	return \"movd   %1,%0\";

      if (GET_CODE (operands[1]) == REG) /* r -> f */
	return \"movld  %1,%0\";

      return \"loadd  %1,%0\";		/* m -> f */
    }

  if (FP_REG_P (operands[1]))
    {
      if (GET_CODE (operands[0]) == REG) /* f -> r */
	return \"movdl  %1,%0\";

      abort ();
    }

  if (GET_CODE (operands[1]) == MEM)	/* m -> r */
    {
      rtx xops[4];
      xops[0] = operands[0];
      xops[1] = gen_rtx (REG, SImode, REGNO (operands[0]) + 1);
      xops[2] = operands[1];
      xops[3] = adj_offsettable_operand (operands[1], 4);
      output_asm_insn (\"loadw  %2,%0\;loadw  %3,%1\", xops);
      return \"\";
    }

  if (GET_CODE (operands[1]) == REG)	/* r -> r */
    {
      rtx xops[4];
      xops[0] = operands[0];
      xops[1] = gen_rtx (REG, SImode, REGNO (operands[0]) + 1);
      xops[2] = operands[1];
      xops[3] = gen_rtx (REG, SImode, REGNO (operands[1]) + 1);
      output_asm_insn (\"movw   %2,%0\;movw   %3,%1\", xops);
      return \"\";
    }

  abort ();
#undef FP_REG_P
}")


(define_insn ""
  [(set (match_operand:DF 0 "memory_operand" "=o,m")
	(match_operand:DF 1 "register_operand" "rf,f"))]
  ""
  "*
{
  rtx xops[4];

  if (REGNO (operands[1]) >= 16)	/* f -> m */
    return \"stord  %1,%0\";

  xops[0] = operands[0];		/* r -> o */
  xops[1] = adj_offsettable_operand (operands[0], 4);
  xops[2] = operands[1];
  xops[3] = gen_rtx (REG, SImode, REGNO (operands[1]) + 1);
  output_asm_insn (\"storw  %2,%0\;storw  %3,%1\", xops);
  return \"\";
}"
[(set_attr "type" "store,store")
 (set_attr "cc" "clobber,unchanged")])


(define_expand "movsf"
  [(set (match_operand:SF 0 "general_operand" "")
	(match_operand:SF 1 "general_operand" ""))]
  ""
  "
{
  if (GET_CODE (operands[0]) == MEM)
    {
      if (GET_CODE (operands[1]) == CONST_DOUBLE)
	operands[1] = force_reg (SFmode,
				 force_const_mem (SFmode, operands[1]));
      else if (GET_CODE (operands[1]) != REG)
	operands[1] = force_reg (SFmode, operands[1]);
    }

  else if (GET_CODE (operands[1]) == CONST_DOUBLE)
    operands[1] = force_const_mem (SFmode, operands[1]);
}")

;;
;; provide two patterns with different predicates as we don't want combine
;; to recombine a mem -> mem move
;; 
(define_insn ""
  [(set (match_operand:SF 0 "register_operand" "=rf")
	(match_operand:SF 1 "nonimmediate_operand" "rfm"))]
  ""
  "*
{
#define FP_REG_P(X) (GET_CODE (X) == REG && REGNO (X) >= 16)

  if (FP_REG_P (operands[0]))
    {
      if (FP_REG_P (operands[1]))	/* f -> f */
	return \"movs   %1,%0\";
      if (GET_CODE (operands[1]) == REG) /* r -> f */
	return
	  \"subq   $8,sp\;storw  %1,(sp)\;loads  (sp),%0\;addq   $8,sp\";
      return \"loads  %1,%0\";		/* m -> f */
    }

  if (FP_REG_P (operands[1]))
    {
      if (GET_CODE (operands[0]) == REG) /* f -> r */
	return
	  \"subq   $8,sp\;stors  %1,(sp)\;loadw  (sp),%0\;addq   $8,sp\";
      abort ();
    }

  if (GET_CODE (operands[1]) == MEM)	/* m -> r */
    return \"loadw   %1,%0\";

  if (GET_CODE (operands[1]) == REG)	/* r -> r */
    return \"movw    %1,%0\";

  abort ();
#undef FP_REG_P
}")

(define_insn ""
  [(set (match_operand:SF 0 "memory_operand" "=m")
	(match_operand:SF 1 "register_operand" "rf"))]
  ""
  "*
{
  if (GET_CODE (operands[1]) == REG && REGNO (operands[1]) >= 16)
    return \"stors  %1,%0\";		/* f-> m */

  return \"storw   %1,%0\";		/* r -> m */
}"
[(set_attr "type" "store")])


(define_expand "movdi"
  [(set (match_operand:DI 0 "general_operand" "")
	(match_operand:DI 1 "general_operand" ""))]
  ""
  "
{
  if (GET_CODE (operands[0]) == MEM && GET_CODE (operands[1]) != REG)
    operands[1] = force_reg (DImode, operands[1]);
}")

(define_insn ""
  [(set (match_operand:DI 0 "register_operand" "=r,r,r")
	(match_operand:DI 1 "general_operand"   "r,n,o"))]
  ""
  "*
{
  rtx xoperands[2],yoperands[2];

  xoperands[0] = gen_rtx (REG, SImode, REGNO (operands[0]) + 1);

  if (which_alternative == 0)		/* r -> r */
    {
      output_asm_insn (\"movw   %1,%0\", operands);
      xoperands[1] = gen_rtx (REG, SImode, REGNO (operands[1]) + 1);
      output_asm_insn (\"movw   %1,%0\", xoperands);
      return \"\";
    }

  if (which_alternative == 1)		/* n -> r */
    {
      if (GET_CODE (operands[1]) == CONST_INT)
	{
	  output_asm_insn (\"loadi   %1,%0\", operands);
	  output_asm_insn (\"loadq   $0,%0\", xoperands);
	  return \"\";
	}

      if (GET_CODE (operands[1]) != CONST_DOUBLE)
	abort ();

      yoperands[0] = operands[0];
      yoperands[1] = gen_rtx (CONST_INT, VOIDmode,
			      CONST_DOUBLE_LOW (operands[1]));
      output_asm_insn (\"loadi  %1,%0\", yoperands);

      xoperands[1] = gen_rtx (CONST_INT, VOIDmode,
			      CONST_DOUBLE_HIGH (operands[1]));
      output_asm_insn (\"loadi  %1,%0\", xoperands);
      return \"\";
    }
					/* m -> r */
  output_asm_insn (\"loadw  %1,%0\", operands);
  xoperands[1] = adj_offsettable_operand (operands[1], 4);
  output_asm_insn (\"loadw  %1,%0\", xoperands);
  return \"\";
}" 
[(set_attr "type" "arith,arith,load")
  (set_attr "cc" "clobber,clobber,clobber")])

(define_insn ""
  [(set (match_operand:DI 0 "memory_operand" "=o")
	(match_operand:DI 1 "register_operand" "r"))]
  ""
  "*
{
  rtx xops[4];
  xops[0] = operands[0];
  xops[1] = adj_offsettable_operand (operands[0], 4);
  xops[2] = operands[1];
  xops[3] = gen_rtx (REG, SImode, REGNO (operands[1]) + 1);
  output_asm_insn (\"storw  %2,%0\;storw  %3,%1\", xops);
  return \"\";
}"
[(set_attr "type" "store")
 (set_attr "cc" "clobber")])

(define_expand "movsi"
  [(set (match_operand:SI 0 "general_operand" "")
	(match_operand:SI 1 "general_operand" ""))]
  ""
  "
{
  if (GET_CODE (operands[0]) == MEM &&
      GET_CODE (operands[1]) != REG)
    operands[1] = force_reg (SImode, operands[1]);
}")

;; provide 2 patterns with different predicates as 'general_operand' in both
;; positions results in a 'mem -> mem' move from combine that must be reloaded 
;;

(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=r,r,r,r")
	(match_operand:SI 1 "general_operand"   "r,m,n,i"))]
  ""
  "*
{
  int val;

  if (which_alternative == 0)
    return \"movw   %1,%0\";		/* reg -> reg */

  if (which_alternative == 1)
    return \"loadw  %1,%0\";		/* mem -> reg */

  if (which_alternative == 2)
    {
      val = INTVAL (operands[1]);	/* known const ->reg */

      if (val == -1)
	return \"notq   $0,%0\";

      if (val < 0 || val >= 16)
	return \"loadi  %1,%0\";

      return \"loadq  %1,%0\";
    }

  if (which_alternative == 3)		/* unknown const */
    return \"loada  %a1,%0\";
}"
[(set_attr "type" "arith,load,arith,load")
 (set_attr "cc" "set2,change0,set1,change0")])


(define_insn ""
  [(set (match_operand:SI 0 "memory_operand" "=m")
	(match_operand:SI 1 "int_reg_operand" "r"))]
  ""
  "storw  %1,%0"
[(set_attr "type" "store")])

;; movhi
;;
;; loadh  mem to reg
;; storh  reg to mem
;;
;;
(define_expand "movhi"
  [(set (match_operand:HI 0 "general_operand" "")
	(match_operand:HI 1 "general_operand" ""))]
  ""
  "
{
  if (GET_CODE (operands[0]) == MEM
      && ! register_operand (operands[1], HImode))
    operands[1] = force_reg (HImode, operands[1]);
}")


(define_insn ""
  [(set (match_operand:HI 0 "register_operand" "=r,r,r")
	(match_operand:HI 1 "general_operand"   "r,m,n"))]
  ""
  "@
   movw   %1,%0
   loadh  %1,%0
   loadi  %1,%0"
[(set_attr "type" "arith,load,arith")])

(define_insn ""
  [(set (match_operand:HI 0 "memory_operand"  "=m")
	(match_operand:HI 1 "register_operand" "r"))]
  ""
  "storh  %1,%0"
 [(set_attr "type" "store")])

;; movqi
;;
;; loadb  mem to reg
;; storb  reg to mem
;;
(define_expand "movqi"
  [(set (match_operand:QI 0 "general_operand" "")
	(match_operand:QI 1 "general_operand" ""))]
  ""
  "
{
  if (GET_CODE (operands[0]) == MEM && 
      ! register_operand (operands[1], QImode))
    operands[1] = force_reg (QImode, operands[1]);
}")


(define_insn ""
  [(set (match_operand:QI 0 "register_operand" "=r,r,r")
	(match_operand:QI 1 "general_operand"   "r,m,n"))]
  ""
  "@
   movw   %1,%0
   loadb  %1,%0
   loadi  %1,%0"
[(set_attr "type" "arith,load,arith")])

(define_insn ""
  [(set (match_operand:QI 0 "memory_operand" "=m")
	(match_operand:QI 1 "register_operand" "r"))]
  ""
  "storb  %1,%0"
[(set_attr "type" "store")])


;;
;; block move
;;
(define_expand "movstrsi"
  [(parallel
    [(set (match_operand:BLK 0 "memory_operand" "")
          (match_operand:BLK 1 "memory_operand" ""))
     (use (match_operand:SI 2 "general_operand" ""))
     (use (match_operand:SI 3 "const_int_operand" ""))
     (clobber (match_scratch:SI 4 ""))
     (clobber (match_scratch:SI 5 ""))
     (clobber (match_dup 6))
     (clobber (match_dup 7))])]
  ""
  "
{
  rtx addr0, addr1;

  addr0 = copy_to_mode_reg (Pmode, XEXP (operands[0], 0));
  addr1 = copy_to_mode_reg (Pmode, XEXP (operands[1], 0));

  operands[6] = addr0;
  operands[7] = addr1;

  operands[0] = gen_rtx (MEM, BLKmode, addr0);
  operands[1] = gen_rtx (MEM, BLKmode, addr1);

  if (GET_CODE (operands[2]) != CONST_INT)
    operands[2] = force_reg (SImode, operands[2]);
}")

;;
;; there is a problem with this insn in gcc-2.2.3
;; (clobber (match_dup 2)) does not prevent use of this operand later
;; we always use a scratch register and leave operand 2 unchanged
;;
(define_insn ""
  [(set (mem:BLK (match_operand:SI 0 "register_operand" "r"))
	(mem:BLK (match_operand:SI 1 "register_operand" "r")))
   (use (match_operand:SI 2 "nonmemory_operand" "rn"))
   (use (match_operand:SI 3 "const_int_operand" "n"))
   (clobber (match_scratch:SI 4 "=r"))
   (clobber (match_scratch:SI 5 "=r"))
   (clobber (match_dup 0))
   (clobber (match_dup 1))]
  ""
  "*
{
  extern void clipper_movstr ();
  clipper_movstr (operands);
  return \"\";
}"
[(set_attr "cc" "clobber")])



;; Extension and truncation insns.
(define_insn "extendhisi2"
  [(set (match_operand:SI 0 "int_reg_operand" "=r,r")
	(sign_extend:SI (match_operand:HI 1 "general_operand" "0,m")))]
  ""
  "@
   andi   $65535,%0\;xori   $32768,%0\;subi   $32768,%0
   loadh  %1,%0"
[(set_attr "type" "arith,load")])


(define_insn "extendqihi2"
  [(set (match_operand:HI 0 "int_reg_operand" "=r,r")
	(sign_extend:HI (match_operand:QI 1 "general_operand" "0,m")))]
  ""
  "@
   andi   $255,%0\;xori   $128,%0\;subi   $128,%0
   loadb  %1,%0"
[(set_attr "type" "arith,load")
 (set_attr "cc" "set1,change0")])


(define_insn "extendqisi2"
  [(set (match_operand:SI 0 "int_reg_operand" "=r,r")
	(sign_extend:SI (match_operand:QI 1 "general_operand" "0,m")))]
  ""
  "@
   andi   $255,%0\;xori   $128,%0\;subi   $128,%0
   loadb  %1,%0"
[(set_attr "type" "arith,load")])


(define_insn "extendsfdf2"
  [(set (match_operand:DF 0 "fp_reg_operand" "=f")
	(float_extend:DF (match_operand:SF 1 "fp_reg_operand" "f")))]
  ""
  "cnvsd  %1,%0")

(define_insn "truncdfsf2"
  [(set (match_operand:SF 0 "fp_reg_operand" "=f")
	(float_truncate:SF (match_operand:DF 1 "fp_reg_operand" "f")))]
  ""
  "cnvds  %1,%0")

(define_insn "zero_extendhisi2"
  [(set (match_operand:SI 0 "int_reg_operand" "=r,r")
	(zero_extend:SI (match_operand:HI 1 "general_operand" "0,m")))]
  ""
  "@
   andi   $65535,%0
   loadhu %1,%0"
[(set_attr "type" "arith,load")])


(define_insn "zero_extendqihi2"
  [(set (match_operand:HI 0 "int_reg_operand" "=r,r")
	(zero_extend:HI (match_operand:QI 1 "general_operand" "0,m")))]
  ""
  "@
   andi   $255,%0
   loadbu %1,%0"
[(set_attr "type" "arith,load")
 (set_attr "cc" "clobber,clobber")])


(define_insn "zero_extendqisi2"
  [(set (match_operand:SI 0 "int_reg_operand" "=r,r")
	(zero_extend:SI (match_operand:QI 1 "general_operand" "0,m")))]
  ""
  "@
   andi   $255,%0
   loadbu %1,%0"
[(set_attr "type" "arith,load")])



;; Fix-to-float conversion insns.

(define_insn "floatsisf2"
  [(set (match_operand:SF 0 "fp_reg_operand" "=f")
	(float:SF (match_operand:SI 1 "int_reg_operand" "r")))]
  ""
  "cnvws  %1,%0")

(define_insn "floatsidf2"
  [(set (match_operand:DF 0 "fp_reg_operand" "=f")
	(float:DF (match_operand:SI 1 "int_reg_operand" "r")))]
  ""
  "cnvwd  %1,%0")


;; Float-to-fix conversion insns.

(define_insn "fix_truncsfsi2"
  [(set (match_operand:SI 0 "int_reg_operand" "=r")
	(fix:SI (fix:SF (match_operand:SF 1 "fp_reg_operand" "f"))))]
  ""
  "cnvtsw %1,%0")

(define_insn "fix_truncdfsi2"
  [(set (match_operand:SI 0 "int_reg_operand" "=r")
	(fix:SI (fix:DF (match_operand:DF 1 "fp_reg_operand" "f"))))]
  ""
  "cnvtdw %1,%0")

;;- All kinds of add instructions.

(define_insn "adddf3"
  [(set (match_operand:DF 0 "fp_reg_operand" "=f")
	(plus:DF (match_operand:DF 1 "fp_reg_operand" "0")
		 (match_operand:DF 2 "fp_reg_operand" "f")))]
  ""
  "addd   %2,%0"
 [(set_attr "type" "fp")])


(define_insn "addsf3"
  [(set (match_operand:SF 0 "fp_reg_operand" "=f")
	(plus:SF (match_operand:SF 1 "fp_reg_operand" "0")
		 (match_operand:SF 2 "fp_reg_operand" "f")))]
  ""
  "adds   %2,%0"
 [(set_attr "type" "fp")])

(define_insn "adddi3"
  [(set (match_operand:DI 0 "int_reg_operand" "=r")
	(plus:DI (match_operand:DI 1 "int_reg_operand" "%0")
		 (match_operand:DI 2 "int_reg_operand" "r")))]
  ""
  "*
{
  rtx xoperands[4];

  xoperands[0] = operands[0];
  xoperands[1] = gen_rtx (REG, SImode, REGNO (operands[0]) + 1);
  xoperands[2] = operands[2];
  xoperands[3] = gen_rtx (REG, SImode, REGNO (operands[2]) + 1);
  output_asm_insn (\"addw   %2,%0\;addwc  %3,%1\", xoperands);
  return \"\";
}"
[(set_attr "type" "arith")
 (set_attr "cc" "clobber")])

(define_insn "addsi3"
  [(set (match_operand:SI 0 "int_reg_operand" "=r,r,r")
	(plus:SI (match_operand:SI 1 "int_reg_operand" "%0,r,r")
		 (match_operand:SI 2 "nonmemory_operand" "rn,0,rn")))]
  ""
  "*
{
  if (which_alternative == 2)		/* 3 address version */
    {
      if (GET_CODE (operands[2]) == CONST_INT)
	return \"loada  %a2(%1),%0\";
      return \"loada  [%2](%1),%0\";
    }
					/* 2 address version */
  if (GET_CODE (operands[2]) == CONST_INT)
    {
      int val = INTVAL (operands[2]);

      if (val >= 16 || val == 0x80000000)
	return \"addi   %2,%0\";

      if (val < 0)			/* change to sub */
	{
	  rtx xops[2];

	  val = -val;

	  xops[0] = operands[0];
	  xops[1] = gen_rtx (CONST_INT, VOIDmode, val);

	  if (val >= 16)
	    output_asm_insn (\"subi   %1,%0\", xops);
	  else
	    output_asm_insn (\"subq   %1,%0\", xops);

	  return \"\";
	}

      return \"addq   %2,%0\";
    }

  if (which_alternative == 0)
    return \"addw   %2,%0\";

  return \"addw   %1,%0\";
}"
[(set_attr "type" "arith,arith,arith")
 (set_attr "cc" "set1,set1,change0")])


;;- All kinds of subtract instructions.

(define_insn "subdi3"
  [(set (match_operand:DI 0 "int_reg_operand" "=r")
	(minus:DI (match_operand:DI 1 "int_reg_operand" "%0")
		  (match_operand:DI 2 "int_reg_operand" "r")))]
  ""
  "*
{
  rtx xoperands[4];

  xoperands[0] = operands[0];
  xoperands[1] = gen_rtx (REG, SImode, REGNO (operands[0]) + 1);
  xoperands[2] = operands[2];
  xoperands[3] = gen_rtx (REG, SImode, REGNO (operands[2]) + 1);
  output_asm_insn (\"subw   %2,%0\;subwc  %3,%1\", xoperands);
  return \"\";
}"
[(set_attr "type" "arith")
 (set_attr "cc" "clobber")])

(define_insn "subsi3"
  [(set (match_operand:SI 0 "int_reg_operand" "=r")
	(minus:SI (match_operand:SI 1 "int_reg_operand" "0")
		  (match_operand:SI 2 "nonmemory_operand" "rn")))]
  ""
  "*
{
  if (GET_CODE (operands[2]) == CONST_INT)
    {
      int val = INTVAL (operands[2]);

      if (val < 0 || val >= 16)
	return \"subi   %2,%0\";
      else
	return \"subq   %2,%0\";
    }

  return \"subw   %2,%0\";
}"
[(set_attr "type" "arith")])

(define_insn "subdf3"
  [(set (match_operand:DF 0 "fp_reg_operand" "=f")
	(minus:DF (match_operand:DF 1 "fp_reg_operand" "0")
		  (match_operand:DF 2 "fp_reg_operand" "f")))]
  ""
  "subd   %2,%0"
 [(set_attr "type" "fp")])

(define_insn "subsf3"
  [(set (match_operand:SF 0 "fp_reg_operand" "=f")
	(minus:SF (match_operand:SF 1 "fp_reg_operand" "0")
		  (match_operand:SF 2 "fp_reg_operand" "f")))]
  ""
  "subs   %2,%0"
 [(set_attr "type" "fp")])


;;- Multiply instructions.

(define_insn "muldf3"
  [(set (match_operand:DF 0 "fp_reg_operand" "=f")
	(mult:DF (match_operand:DF 1 "fp_reg_operand" "0")
		 (match_operand:DF 2 "fp_reg_operand" "f")))]
  ""
  "muld   %2,%0"
 [(set_attr "type" "fp")])

(define_insn "mulsf3"
  [(set (match_operand:SF 0 "fp_reg_operand" "=f")
	(mult:SF (match_operand:SF 1 "fp_reg_operand" "0")
		 (match_operand:SF 2 "fp_reg_operand" "f")))]
  ""
  "muls   %2,%0"
 [(set_attr "type" "fp")])

(define_insn "mulsidi3"
  [(set (match_operand:DI 0 "int_reg_operand" "=r")
	(mult:DI (sign_extend:DI (match_operand:SI 1 "int_reg_operand" "%0"))
	         (sign_extend:DI (match_operand:SI 2 "int_reg_operand" "r"))))]
  ""
  "mulwx  %2,%0"
[(set_attr "type" "arith")
 (set_attr "cc" "clobber")])

(define_insn "umulsidi3"
  [(set (match_operand:DI 0 "int_reg_operand" "=r")
	(mult:DI (zero_extend:DI (match_operand:SI 1 "int_reg_operand" "%0"))
	         (zero_extend:DI (match_operand:SI 2 "int_reg_operand" "r"))))]
  ""
  "mulwux %2,%0"
[(set_attr "type" "arith")
 (set_attr "cc" "clobber")])

(define_insn "mulsi3"
  [(set (match_operand:SI 0 "int_reg_operand" "=r")
	(mult:SI (match_operand:SI 1 "int_reg_operand" "%0")
	         (match_operand:SI 2 "int_reg_operand" "r")))]
  ""
  "mulw   %2,%0"
 [(set_attr "type" "arith")
  (set_attr "cc" "clobber")])


;;- Divide and mod instructions.

(define_insn "divdf3"
  [(set (match_operand:DF 0 "fp_reg_operand" "=f")
	(div:DF (match_operand:DF 1 "fp_reg_operand" "0")
		(match_operand:DF 2 "fp_reg_operand" "f")))]
  ""
  "divd   %2,%0"
 [(set_attr "type" "fp")])

(define_insn "divsf3"
  [(set (match_operand:SF 0 "fp_reg_operand" "=f")
	(div:SF (match_operand:SF 1 "fp_reg_operand" "0")
		(match_operand:SF 2 "fp_reg_operand" "f")))]
  ""
  "divs   %2,%0"
 [(set_attr "type" "fp")])

(define_insn "divsi3"
  [(set (match_operand:SI 0 "int_reg_operand" "=r")
	(div:SI (match_operand:SI 1 "int_reg_operand" "0")
		(match_operand:SI 2 "int_reg_operand" "r")))]
  ""
  "divw   %2,%0"
 [(set_attr "type" "arith")
  (set_attr "cc" "clobber")])

(define_insn "udivsi3"
  [(set (match_operand:SI 0 "int_reg_operand" "=r")
	(udiv:SI (match_operand:SI 1 "int_reg_operand" "0")
	         (match_operand:SI 2 "int_reg_operand" "r")))]
  ""
  "divwu  %2,%0"
 [(set_attr "type" "arith")
  (set_attr "cc" "clobber")])


(define_insn "modsi3"
  [(set (match_operand:SI 0 "int_reg_operand" "=r")
	(mod:SI (match_operand:SI 1 "int_reg_operand" "0")
		(match_operand:SI 2 "int_reg_operand" "r")))]
  ""
  "modw   %2,%0"
 [(set_attr "type" "arith")
  (set_attr "cc" "clobber")])

(define_insn "umodsi3"
  [(set (match_operand:SI 0 "int_reg_operand" "=r")
	(umod:SI (match_operand:SI 1 "int_reg_operand" "0")
	         (match_operand:SI 2 "int_reg_operand" "r")))]
  ""
  "modwu  %2,%0"
 [(set_attr "type" "arith")
  (set_attr "cc" "clobber")])

;;
;; bit and/or instructions
;;
(define_insn "andsi3"
  [(set (match_operand:SI 0 "int_reg_operand" "=r,r")
        (and:SI (match_operand:SI 1 "int_reg_operand" "%0,0")
		(match_operand:SI 2 "nonmemory_operand" "r,n")))]
  ""
  "@
   andw   %2,%0
   andi   %2,%0"
 [(set_attr "type" "arith")])

(define_insn "iorsi3"
  [(set (match_operand:SI 0 "int_reg_operand" "=r,r")
	(ior:SI (match_operand:SI 1 "int_reg_operand" "%0,0")
	        (match_operand:SI 2 "nonmemory_operand" "r,n")))]
  ""
  "@
   orw    %2,%0
   ori    %2,%0"
 [(set_attr "type" "arith")])

(define_insn "xorsi3"
  [(set (match_operand:SI 0 "int_reg_operand" "=r,r")
	(xor:SI (match_operand:SI 1 "int_reg_operand" "%0,0")
		(match_operand:SI 2 "nonmemory_operand" "r,n")))]
  ""
  "@
   xorw   %2,%0
   xori   %2,%0"
 [(set_attr "type" "arith")])

(define_insn "negdf2"
  [(set (match_operand:DF 0 "fp_reg_operand" "=f")
	(neg:DF (match_operand:DF 1 "fp_reg_operand" "f")))]
  ""
  "negd   %1,%0"
 [(set_attr "type" "fp")])

(define_insn "negsf2"
  [(set (match_operand:SF 0 "fp_reg_operand" "=f")
	(neg:SF (match_operand:SF 1 "fp_reg_operand" "f")))]
  ""
  "negs   %1,%0"
 [(set_attr "type" "fp")])

(define_insn "negsi2"
  [(set (match_operand:SI 0 "int_reg_operand" "=r")
	(neg:SI (match_operand:SI 1 "int_reg_operand" "r")))]
  ""
  "negw   %1,%0"
 [(set_attr "type" "arith")])


(define_insn "one_cmplsi2"
  [(set (match_operand:SI 0 "int_reg_operand" "=r")
	(not:SI (match_operand:SI 1 "int_reg_operand" "r")))]
  ""
  "notw   %1,%0"
 [(set_attr "type" "arith")])



;; Right shift on the clipper works by negating the shift count,
;; then emitting a right shift with the shift count negated.  This means
;; that all actual shift counts in the RTL will be positive.

(define_expand "ashrdi3"
  [(set (match_operand:DI 0 "int_reg_operand" "")
	(ashiftrt:DI (match_operand:DI 1 "int_reg_operand" "")
	             (match_operand:SI 2 "nonmemory_operand" "")))]
  ""
  "
{
  if (GET_CODE (operands[2]) != CONST_INT)
    operands[2] = gen_rtx (NEG, SImode, negate_rtx (SImode, operands[2]));
}")

(define_insn ""
  [(set (match_operand:DI 0 "int_reg_operand" "=r")
	(ashiftrt:DI (match_operand:DI 1 "int_reg_operand" "0")
		     (match_operand:SI 2 "const_int_operand" "n")))]
  ""
  "shali  $%n2,%0"
 [(set_attr "type" "arith")])

(define_insn ""
  [(set (match_operand:DI 0 "int_reg_operand" "=r")
	(ashiftrt:DI (match_operand:DI 1 "int_reg_operand" "0")
		     (neg:SI (match_operand:SI 2 "nonmemory_operand" "r"))))]
  ""
  "shal   %2,%0"
 [(set_attr "type" "arith")])

(define_expand "ashrsi3"
  [(set (match_operand:SI 0 "int_reg_operand" "")
	(ashiftrt:SI (match_operand:SI 1 "int_reg_operand" "")
	             (match_operand:SI 2 "nonmemory_operand" "")))]
  ""
  "
{
  if (GET_CODE (operands[2]) != CONST_INT)
    operands[2] = gen_rtx (NEG, SImode, negate_rtx (SImode, operands[2]));
}")

(define_insn ""
  [(set (match_operand:SI 0 "int_reg_operand" "=r")
	(ashiftrt:SI (match_operand:SI 1 "int_reg_operand" "0")
		     (match_operand:SI 2 "const_int_operand" "n")))]
  ""
  "shai   $%n2,%0"
 [(set_attr "type" "arith")])

(define_insn ""
  [(set (match_operand:SI 0 "int_reg_operand" "=r")
	(ashiftrt:SI (match_operand:SI 1 "int_reg_operand" "0")
		     (neg:SI (match_operand:SI 2 "nonmemory_operand" "r"))))]
  ""
  "shaw   %2,%0"
 [(set_attr "type" "arith")])

;;
;; left shift
;;

(define_insn "ashldi3"
  [(set (match_operand:DI 0 "int_reg_operand" "=r,r")
	(ashift:DI (match_operand:DI 1 "int_reg_operand" "0,0")
		   (match_operand:SI 2 "nonmemory_operand" "r,n")))]
  ""
  "@
   shal   %2,%0
   shali  %2,%0"
 [(set_attr "type" "arith")])


(define_insn "ashlsi3"
  [(set (match_operand:SI 0 "int_reg_operand" "=r,r")
	(ashift:SI (match_operand:SI 1 "int_reg_operand" "0,0")
		   (match_operand:SI 2 "nonmemory_operand" "r,n")))]
  ""
  "*
{
  int val;

  if (which_alternative == 0)
   return \"shaw   %2,%0\";

  val = INTVAL (operands[2]);

  if (val == 2)
    return \"addw   %0,%0\;addw   %0,%0\";

  if (val == 1)
    return \"addw   %0,%0\";

  return \"shai   %2,%0\";
}"
[(set_attr "type" "arith")])

;;
;; logical shift
;;

(define_expand "lshrdi3"
  [(set (match_operand:DI 0 "int_reg_operand" "")
	(lshiftrt:DI (match_operand:DI 1 "int_reg_operand" "")
	             (match_operand:SI 2 "nonmemory_operand" "")))]
  ""
  "
{
  if (GET_CODE (operands[2]) != CONST_INT)
    operands[2] = gen_rtx (NEG, SImode, negate_rtx (SImode, operands[2]));
}")

(define_insn ""
  [(set (match_operand:DI 0 "int_reg_operand" "=r")
	(lshiftrt:DI (match_operand:DI 1 "int_reg_operand" "0")
		     (match_operand:SI 2 "const_int_operand" "n")))]
  ""
  "shlli  $%n2,%0"
 [(set_attr "type" "arith")])

(define_insn ""
  [(set (match_operand:DI 0 "int_reg_operand" "=r")
	(lshiftrt:DI (match_operand:DI 1 "int_reg_operand" "0")
		     (neg:SI (match_operand:SI 2 "nonmemory_operand" "r"))))]
  ""
  "shll   %2,%0"
 [(set_attr "type" "arith")])

(define_expand "lshrsi3"
  [(set (match_operand:SI 0 "int_reg_operand" "")
	(lshiftrt:SI (match_operand:SI 1 "int_reg_operand" "")
	             (match_operand:SI 2 "nonmemory_operand" "")))]
  ""
  "
{
  if (GET_CODE (operands[2]) != CONST_INT)
    operands[2] = gen_rtx (NEG, SImode, negate_rtx (SImode, operands[2]));
}")

(define_insn ""
  [(set (match_operand:SI 0 "int_reg_operand" "=r")
	(lshiftrt:SI (match_operand:SI 1 "int_reg_operand" "0")
		     (match_operand:SI 2 "const_int_operand" "n")))]
  ""
  "shli   $%n2,%0"
 [(set_attr "type" "arith")])

(define_insn ""
  [(set (match_operand:SI 0 "int_reg_operand" "=r")
	(lshiftrt:SI (match_operand:SI 1 "int_reg_operand" "0")
		     (neg:SI (match_operand:SI 2 "nonmemory_operand" "r"))))]
  ""
  "shlw   %2,%0"
 [(set_attr "type" "arith")])

(define_insn "lshldi3"
  [(set (match_operand:DI 0 "int_reg_operand" "=r,r")
	(lshift:DI (match_operand:DI 1 "int_reg_operand" "0,0")
		   (match_operand:SI 2 "nonmemory_operand" "r,n")))]
  ""
  "@
   shll   %2,%0
   shlli  %2,%0"
 [(set_attr "type" "arith")])

(define_insn "lshlsi3"
  [(set (match_operand:SI 0 "int_reg_operand" "=r,r")
	(lshift:SI (match_operand:SI 1 "int_reg_operand" "0,0")
		   (match_operand:SI 2 "nonmemory_operand" "r,n")))]
  ""
  "@
   shlw   %2,%0
   shli   %2,%0"
 [(set_attr "type" "arith")])

;;
;; rotate insn
;;
(define_expand "rotrdi3"
  [(set (match_operand:DI 0 "int_reg_operand" "")
	(rotatert:DI (match_operand:DI 1 "int_reg_operand" "")
	             (match_operand:SI 2 "nonmemory_operand" "")))]
  ""
  "
{
  if (GET_CODE (operands[2]) != CONST_INT)
    operands[2] = gen_rtx (NEG, SImode, negate_rtx (SImode, operands[2]));
}")

(define_insn ""
  [(set (match_operand:DI 0 "int_reg_operand" "=r")
	(rotatert:DI (match_operand:DI 1 "int_reg_operand" "0")
		     (match_operand:SI 2 "const_int_operand" "n")))]
  ""
  "rotli  $%n2,%0"
 [(set_attr "type" "arith")])

(define_insn ""
  [(set (match_operand:DI 0 "int_reg_operand" "=r")
	(rotatert:DI (match_operand:DI 1 "int_reg_operand" "0")
		     (neg:SI (match_operand:SI 2 "nonmemory_operand" "r"))))]
  ""
  "rotl   %2,%0"
 [(set_attr "type" "arith")])

(define_expand "rotrsi3"
  [(set (match_operand:SI 0 "int_reg_operand" "")
	(rotatert:SI (match_operand:SI 1 "int_reg_operand" "")
	             (match_operand:SI 2 "nonmemory_operand" "")))]
  ""
  "
{
  if (GET_CODE (operands[2]) != CONST_INT)
    operands[2] = gen_rtx (NEG, SImode, negate_rtx (SImode, operands[2]));
}")

(define_insn ""
  [(set (match_operand:SI 0 "int_reg_operand" "=r")
	(rotatert:SI (match_operand:SI 1 "int_reg_operand" "0")
		     (match_operand:SI 2 "const_int_operand" "n")))]
  ""
  "roti   $%n2,%0"
 [(set_attr "type" "arith")])

(define_insn ""
  [(set (match_operand:SI 0 "int_reg_operand" "=r")
	(rotatert:SI (match_operand:SI 1 "int_reg_operand" "0")
		     (neg:SI (match_operand:SI 2 "nonmemory_operand" "r"))))]
  ""
  "rotw   %2,%0"
 [(set_attr "type" "arith")])

(define_insn "rotldi3"
  [(set (match_operand:DI 0 "int_reg_operand" "=r,r")
	(rotate:DI (match_operand:DI 1 "int_reg_operand" "0,0")
		   (match_operand:SI 2 "nonmemory_operand" "r,n")))]
  ""
  "@
   rotl   %2,%0
   rotli  %2,%0"
 [(set_attr "type" "arith")])

(define_insn "rotlsi3"
  [(set (match_operand:SI 0 "int_reg_operand" "=r,r")
	(rotate:SI (match_operand:SI 1 "int_reg_operand" "0,0")
		   (match_operand:SI 2 "nonmemory_operand" "r,n")))]
  ""
  "@
   rotw   %2,%0
   roti   %2,%0"
 [(set_attr "type" "arith")])


;;
;; jump and branch insns
;;
(define_insn "jump"
  [(set (pc)
	(label_ref (match_operand 0 "" "")))]
  ""
  "b      %l0"
 [(set_attr "type" "branch")])

(define_insn "tablejump"
  [(set (pc) (match_operand:SI 0 "register_operand" "r"))
   (use (label_ref (match_operand 1 "" "")))]
  ""
  "b      (%0)"
 [(set_attr "type" "branch")])

(define_insn "beq"
  [(set (pc)
	(if_then_else (eq (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "breq   %l0"
 [(set_attr "type" "branch")])

(define_insn "bne"
  [(set (pc)
	(if_then_else (ne (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "brne   %l0"
 [(set_attr "type" "branch")])

(define_insn "bgt"
  [(set (pc)
	(if_then_else (gt (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "brgt   %l0"
 [(set_attr "type" "branch")])

(define_insn "bgtu"
  [(set (pc)
	(if_then_else (gtu (cc0)
			   (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "brgtu  %l0"
 [(set_attr "type" "branch")])

(define_insn "blt"
  [(set (pc)
	(if_then_else (lt (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "brlt   %l0"
 [(set_attr "type" "branch")])

(define_insn "bltu"
  [(set (pc)
	(if_then_else (ltu (cc0)
			   (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "brltu  %l0"
 [(set_attr "type" "branch")])

(define_insn "bge"
  [(set (pc)
	(if_then_else (ge (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "brge   %l0"
 [(set_attr "type" "branch")])

(define_insn "bgeu"
  [(set (pc)
	(if_then_else (geu (cc0)
			   (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
  "brgeu  %l0"
 [(set_attr "type" "branch")])

(define_insn "ble"
  [(set (pc)
	(if_then_else (le (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
 ""
 "brle   %l0"
 [(set_attr "type" "branch")])

(define_insn "bleu"
  [(set (pc)
	(if_then_else (leu (cc0)
			   (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
 ""
 "brleu  %l0"
 [(set_attr "type" "branch")])

;; Recognize reversed jumps.
(define_insn ""
  [(set (pc)
	(if_then_else (match_operator 0 "comparison_operator"
				      [(cc0)
				       (const_int 0)])
		      (pc)
		      (label_ref (match_operand 1 "" ""))))]
 ""
 "br%C0    %l1" ; %C0 negates condition
 [(set_attr "type" "branch")])

;;
;; call instructions
;;
(define_insn "call"
  [(call (match_operand:QI 0 "general_operand" "m")
	 (match_operand:SI 1 "general_operand" ""))]
  ;; Operand 1 not used on the clipper.
  ""
  "call   sp,%0")

(define_insn "call_value"
  [(set (match_operand 0 "" "=rf")
	(call (match_operand:QI 1 "general_operand" "m")
	      (match_operand:SI 2 "general_operand" "g")))]
  ;; Operand 2 not used on the clipper
  ""
  "call   sp,%1")

(define_insn "indirect_jump"
  [(set (pc) (match_operand:SI 0 "register_operand" "r"))]
  ""
  "b      (%0)"
 [(set_attr "type" "branch")])


(define_insn "nop"
  [(const_int 0)]
  ""
  "noop"
 [(set_attr "type" "arith")
  (set_attr "cc" "unchanged")])



;; while (--foo >= 0)
;;
;; Combiners for 'decrement test and branch' do not work for clipper.
;; These patters are jump_insns that do not allow output reloads and clipper
;; can only decrement and test registers.
;;
